diff --git a/./drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c.orig b/./drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
index f507d82..6c06044 100644
--- a/./drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c.orig
+++ b/./drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
@@ -2743,6 +2743,8 @@ brcmf_cfg80211_set_power_mgmt(struct wiphy *wiphy, struct net_device *ndev,
 	 * preference in cfg struct to apply this to
 	 * FW later while initializing the dongle
 	 */
+	pr_info("power management disabled\n");
+	enabled = false;
 	cfg->pwr_save = enabled;
 	if (!check_vif_up(ifp->vif)) {
 
