(footprint "L_CommonModeChoke_Panasonic_EXC14CE" (version 20210126) (generator pcbnew) (layer "F.Cu")
  (tedit 60317FFB)
  (descr "Coilcraft 0603USB Series Common Mode Choke, https://www.coilcraft.com/pdfs/0603usb.pdf")
  (tags "surface mount common mode bead")
  (attr smd)
  (fp_text reference "REF**" (at 0 1.7) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bb38d00d-ec04-40de-832b-8e4f1589efd1)
  )
  (fp_text value "L_CommonModeChoke_Panasonic_EXC14CE" (at 0 -2.01) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 56dcc907-2673-43fd-81fb-975b2e0cd033)
  )
  (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
    (effects (font (size 0.5 0.5) (thickness 0.075)))
    (tstamp acb21aad-7748-421c-aabe-12febfab133e)
  )
  (fp_line (start -0.63 -0.5) (end -0.63 0.3) (layer "F.SilkS") (width 0.1) (tstamp 272d177d-9f6c-42f2-8e43-e9aa1d30810c))
  (fp_line (start 0.63 0.3) (end 0.63 -0.3) (layer "F.SilkS") (width 0.1) (tstamp 4ee30f4e-6cda-47fe-b9b4-13f1baea768f))
  (fp_line (start 0.68 0.7) (end 0.68 -0.7) (layer "F.CrtYd") (width 0.05) (tstamp 3c300153-e757-4a1c-8034-dcb6d60f8f94))
  (fp_line (start -0.68 -0.7) (end 0.68 -0.7) (layer "F.CrtYd") (width 0.05) (tstamp 9c412fbb-93e7-4f6b-8ff8-19d045751bcc))
  (fp_line (start -0.68 0.7) (end -0.68 -0.7) (layer "F.CrtYd") (width 0.05) (tstamp b3067c24-0a17-4240-9b08-713169643363))
  (fp_line (start -0.68 0.7) (end 0.68 0.7) (layer "F.CrtYd") (width 0.05) (tstamp e5c7c2b4-2ae5-4a14-86be-faf4ba680779))
  (fp_line (start -0.425 -0.1) (end -0.425 0.325) (layer "F.Fab") (width 0.1) (tstamp 02e44637-f281-4074-94cb-ab2097b51e3f))
  (fp_line (start -0.425 0.325) (end 0.425 0.325) (layer "F.Fab") (width 0.1) (tstamp 03d25992-1100-45c6-bdda-4f8d2635dafc))
  (fp_line (start -0.2 -0.325) (end 0.425 -0.325) (layer "F.Fab") (width 0.1) (tstamp 0a1e3186-e651-436d-a30d-00f2cb137454))
  (fp_line (start 0.425 -0.325) (end 0.425 0.325) (layer "F.Fab") (width 0.1) (tstamp 9b02d5a7-de93-4a0c-b880-3ce25a24e207))
  (fp_line (start -0.425 -0.1) (end -0.2 -0.325) (layer "F.Fab") (width 0.1) (tstamp e172fd65-edba-4fff-a9f0-519e357a97c3))
  (pad "1" smd roundrect (at -0.25 -0.325) (locked) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05) (tstamp b425e555-8af7-4325-a82e-27acc1041b85))
  (pad "2" smd roundrect (at 0.25 -0.325) (locked) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05) (tstamp 40aebfaa-c80f-4a61-b980-a84a5c9a40a0))
  (pad "3" smd roundrect (at 0.25 0.325) (locked) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05) (tstamp 48a38762-b357-4b30-bf43-4bcbc0d21753))
  (pad "4" smd roundrect (at -0.25 0.325) (locked) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05) (tstamp 50efcabf-c4c2-495b-abba-0aa748e4f104))
  (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_CommonModeChoke_Coilcraft_0603USB.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
