(footprint "QFN-28-1EP_4x5mm_P0.5mm_EP2.65x3.65mm_ThermalVias_0.3" (version 20210824) (generator pcbnew) (layer "F.Cu")
  (tedit 6187FD60)
  (descr "QFN, 28 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/3555fe.pdf#page=32), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.82) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f17eeef4-8e17-4672-a52a-e16f66d5eabc)
  )
  (fp_text value "QFN-28-1EP_4x5mm_P0.5mm_EP2.65x3.65mm_ThermalVias_0.3" (at 0 3.82) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b81787ae-9bf8-401b-b4a3-bae6a8d88a7d)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp da921527-7fd9-45b3-a2f0-b9c063fe965e)
  )
  (fp_line (start -1.635 2.61) (end -2.11 2.61) (layer "F.SilkS") (width 0.12) (tstamp 82b70b8d-dd67-495e-a063-b957381ba133))
  (fp_line (start 1.635 -2.61) (end 2.11 -2.61) (layer "F.SilkS") (width 0.12) (tstamp 88c67ac3-0d1b-4ffd-90af-87c9a291e8a7))
  (fp_line (start 2.11 -2.61) (end 2.11 -2.135) (layer "F.SilkS") (width 0.12) (tstamp b5b5a73f-614c-4bc6-a453-cac55d37913b))
  (fp_line (start 2.11 2.61) (end 2.11 2.135) (layer "F.SilkS") (width 0.12) (tstamp c2645db8-7483-411c-9a03-d83bfbb3b7ba))
  (fp_line (start -1.635 -2.61) (end -2.11 -2.61) (layer "F.SilkS") (width 0.12) (tstamp ce44eab4-72b8-4929-a9f7-7ae115fb7753))
  (fp_line (start 1.635 2.61) (end 2.11 2.61) (layer "F.SilkS") (width 0.12) (tstamp f4b4d9dd-02bc-41c9-aede-de5673a70d3e))
  (fp_line (start -2.11 2.61) (end -2.11 2.135) (layer "F.SilkS") (width 0.12) (tstamp fcd3b3fc-016f-49d8-a513-0a2f0e1994bf))
  (fp_line (start -2.62 3.12) (end 2.62 3.12) (layer "F.CrtYd") (width 0.05) (tstamp 04c2c781-7b00-417f-b91b-299dcd2f3023))
  (fp_line (start 2.62 3.12) (end 2.62 -3.12) (layer "F.CrtYd") (width 0.05) (tstamp 5fd1f60c-026d-481c-91f8-2c2997418044))
  (fp_line (start 2.62 -3.12) (end -2.62 -3.12) (layer "F.CrtYd") (width 0.05) (tstamp 769c958f-4292-44a3-99b8-98a2cba44ec6))
  (fp_line (start -2.62 -3.12) (end -2.62 3.12) (layer "F.CrtYd") (width 0.05) (tstamp d700e24f-8bcf-42d6-8189-a62464b04200))
  (fp_line (start -2 -1.5) (end -1 -2.5) (layer "F.Fab") (width 0.1) (tstamp 1003a6af-4680-40f5-a3d3-bf88db15ca74))
  (fp_line (start -2 2.5) (end -2 -1.5) (layer "F.Fab") (width 0.1) (tstamp 1b7cda08-bca2-4d50-93ac-8385d2beebff))
  (fp_line (start -1 -2.5) (end 2 -2.5) (layer "F.Fab") (width 0.1) (tstamp 4c403c8b-8751-4fda-bf52-a2668a9a1a43))
  (fp_line (start 2 -2.5) (end 2 2.5) (layer "F.Fab") (width 0.1) (tstamp 50e0c564-b900-4fe4-885e-3bc5ece9707f))
  (fp_line (start 2 2.5) (end -2 2.5) (layer "F.Fab") (width 0.1) (tstamp db75e9f0-f0a6-4b43-b85a-21cd54d55b50))
  (pad "" smd roundrect locked (at -0.55 1.05) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 46eb214e-b015-4629-9e27-2312cf856b49))
  (pad "" smd roundrect locked (at 0.55 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 799b85b3-ecc5-472e-abb8-bea054e6d1fa))
  (pad "" smd roundrect locked (at -0.55 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 939402bf-1805-4f6f-aa1f-2de15079597f))
  (pad "" smd roundrect locked (at -0.55 -1.05) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp bd616bfc-930a-4e5d-a56a-96e9e93c8c83))
  (pad "" smd roundrect locked (at 0.55 1.05) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp c5507b85-3f56-46f9-bc42-4971df706b49))
  (pad "" smd roundrect locked (at 0.55 -1.05) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp c9655ef6-2803-48ee-b7e0-6b365aabc00e))
  (pad "1" smd roundrect locked (at -1.95 -1.75) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 20b4cb83-5b4c-4e69-bdea-4e58a1a665c5))
  (pad "2" smd roundrect locked (at -1.95 -1.25) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 65ea61df-b7e7-4775-92e5-212413c6b235))
  (pad "3" smd roundrect locked (at -1.95 -0.75) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1548d30e-8434-4143-8c13-9619ed2c971f))
  (pad "4" smd roundrect locked (at -1.95 -0.25) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2331df7a-88a6-421d-8639-92df659818bc))
  (pad "5" smd roundrect locked (at -1.95 0.25) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 51aa5d8f-b445-4cda-9aea-3d84c29c1f63))
  (pad "6" smd roundrect locked (at -1.95 0.75) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9924a91f-2f78-4c9e-9e0f-6efd1c03e79e))
  (pad "7" smd roundrect locked (at -1.95 1.25) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1ac0d445-516d-4e66-a825-8e1841c245ea))
  (pad "8" smd roundrect locked (at -1.95 1.75) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0a1d26f1-9b41-4faa-92ae-db297513a264))
  (pad "9" smd roundrect locked (at -1.25 2.45) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a2ec92b6-baa5-447d-a914-0e6055b355f3))
  (pad "10" smd roundrect locked (at -0.75 2.45) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4de97ffd-6f34-43fb-85c1-51cfbd8d8a2c))
  (pad "11" smd roundrect locked (at -0.25 2.45) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2ff32620-a410-4777-9eb3-d3dfc69bf340))
  (pad "12" smd roundrect locked (at 0.25 2.45) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f1880b46-f8bc-41eb-a36e-587b40c031b9))
  (pad "13" smd roundrect locked (at 0.75 2.45) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 799e4813-6b26-48d0-9fe0-b3a373b00b9d))
  (pad "14" smd roundrect locked (at 1.25 2.45) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 32e4c7b4-4a9b-46ff-b1d2-f630df892a4c))
  (pad "15" smd roundrect locked (at 1.95 1.75) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp daffb7b7-095a-4c39-bacb-3abbc84c7598))
  (pad "16" smd roundrect locked (at 1.95 1.25) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0712832c-6ccc-4445-8605-b9569a8e7bb9))
  (pad "17" smd roundrect locked (at 1.95 0.75) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a090cd56-9f5c-44e1-b40e-ee3b024378a6))
  (pad "18" smd roundrect locked (at 1.95 0.25) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 03432ae6-e130-42d8-a0a9-12b4f6e0652d))
  (pad "19" smd roundrect locked (at 1.95 -0.25) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a85ac759-127c-4176-9cdf-1b2a7ec655a1))
  (pad "20" smd roundrect locked (at 1.95 -0.75) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ea360254-aa93-4814-a0d0-98749d497f7e))
  (pad "21" smd roundrect locked (at 1.95 -1.25) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 05409a5f-f2bb-48b3-8678-3b95e695050d))
  (pad "22" smd roundrect locked (at 1.95 -1.75) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b2a404e3-da86-408c-aedf-c5771c353e60))
  (pad "23" smd roundrect locked (at 1.25 -2.45) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e9558e4c-29a1-40a2-a401-65453a526b99))
  (pad "24" smd roundrect locked (at 0.75 -2.45) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ff5dcbc4-1166-4d9d-9d53-4fe4434f452e))
  (pad "25" smd roundrect locked (at 0.25 -2.45) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6cf48371-39af-43ae-9762-8c72b5e2d16a))
  (pad "26" smd roundrect locked (at -0.25 -2.45) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 449660d2-5ab7-44fb-8090-81537418aead))
  (pad "27" smd roundrect locked (at -0.75 -2.45) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f35bc1ad-0f92-466c-933c-332509bad3ec))
  (pad "28" smd roundrect locked (at -1.25 -2.45) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 331e1c6c-30b6-4431-8f05-e718ca887075))
  (pad "29" thru_hole circle locked (at 1 -0.525) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 06bcd15b-eabd-440d-b4bb-b9d27151cb18))
  (pad "29" thru_hole circle locked (at 0 -0.525) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 2cc2571a-8b20-49c9-a197-598deb5c3868))
  (pad "29" thru_hole circle locked (at -1 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 30e731f4-f3b7-4739-b970-37fae116d871))
  (pad "29" thru_hole circle locked (at -1 0.525) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 390b678f-8624-4f4e-b23d-73260c6508f2))
  (pad "29" smd rect locked (at 0 0) (size 2.65 3.65) (layers "B.Cu") (tstamp 43072768-f0ae-4f24-b851-700dff98009b))
  (pad "29" thru_hole circle locked (at 0 0.525) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 92ce63fd-fc4c-4401-8bc7-8a6b958c8675))
  (pad "29" thru_hole circle locked (at 0 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 948e3652-518d-4706-bcce-796c7d53ea37))
  (pad "29" thru_hole circle locked (at 1 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 9a460f86-2dcb-4dfc-8add-cc8f3481228c))
  (pad "29" thru_hole circle locked (at -1 -0.525) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 9bb612de-bfb5-4ddf-9da6-58698d28e7fa))
  (pad "29" thru_hole circle locked (at 0 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp b5a903e6-b417-4133-b459-603aaae29923))
  (pad "29" thru_hole circle locked (at 1 0.525) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp bcc73795-9961-4e09-94db-a236baa02ded))
  (pad "29" thru_hole circle locked (at 1 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp dbe7c23f-465c-4159-942c-da8386b6625c))
  (pad "29" smd rect locked (at 0 0) (size 2.65 3.65) (layers "F.Cu" "F.Mask") (tstamp ded4bfe4-5276-424a-a999-764cad65a1c3))
  (pad "29" thru_hole circle locked (at -1 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp f5d87a9a-5c19-493d-bf16-51271eb32f76))
  (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-28-1EP_4x5mm_P0.5mm_EP2.65x3.65mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
