(footprint "MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm_ThermalVias_0.3" (version 20210824) (generator pcbnew) (layer "F.Cu")
  (tedit 6187FD06)
  (descr "MSOP, 10 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3805fg.pdf#page=18), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "MSOP SO")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.45) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b0ab9da1-37bb-4274-95ed-09d4466ccfeb)
  )
  (fp_text value "MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm_ThermalVias_0.3" (at 0 2.45) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 541b3eff-2ede-4fb5-82c0-a07ffffa4065)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 0.75 0.75) (thickness 0.11)))
    (tstamp fe4a96eb-0c4f-4b7a-9422-174162a6793c)
  )
  (fp_line (start 0 1.61) (end -1.5 1.61) (layer "F.SilkS") (width 0.12) (tstamp 4db0b1d6-b7c3-497d-b510-abd58e938ab9))
  (fp_line (start 0 -1.61) (end -2.875 -1.61) (layer "F.SilkS") (width 0.12) (tstamp 6bb7d843-c678-4ad7-a51b-ad66460151e8))
  (fp_line (start 0 1.61) (end 1.5 1.61) (layer "F.SilkS") (width 0.12) (tstamp 6f406202-8354-475b-b55d-46fe9780d2ca))
  (fp_line (start 0 -1.61) (end 1.5 -1.61) (layer "F.SilkS") (width 0.12) (tstamp 873c5850-15f3-4d43-a85a-f8565f56acb9))
  (fp_line (start -3.12 1.75) (end 3.12 1.75) (layer "F.CrtYd") (width 0.05) (tstamp 30ab5984-974d-49ad-9912-e371fb59fc1a))
  (fp_line (start 3.12 1.75) (end 3.12 -1.75) (layer "F.CrtYd") (width 0.05) (tstamp 36fc256d-afd1-4cba-b79d-ec6835f0f260))
  (fp_line (start -3.12 -1.75) (end -3.12 1.75) (layer "F.CrtYd") (width 0.05) (tstamp 780b74ad-05a8-4a25-b5d1-6c596978d2dc))
  (fp_line (start 3.12 -1.75) (end -3.12 -1.75) (layer "F.CrtYd") (width 0.05) (tstamp 94337a92-d42b-404b-b741-73f1ad06d861))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer "F.Fab") (width 0.1) (tstamp 10ccad52-0f89-48a8-b877-36795af37296))
  (fp_line (start -0.75 -1.5) (end 1.5 -1.5) (layer "F.Fab") (width 0.1) (tstamp 38438add-e53d-45ff-98e5-0c2ec90a6003))
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer "F.Fab") (width 0.1) (tstamp 5b83c471-9061-4f67-b1e2-72d57603263b))
  (fp_line (start -1.5 1.5) (end -1.5 -0.75) (layer "F.Fab") (width 0.1) (tstamp 6ce602a0-774c-4ea7-9500-b485d6d9fdf8))
  (fp_line (start -1.5 -0.75) (end -0.75 -1.5) (layer "F.Fab") (width 0.1) (tstamp af140e49-5adc-4090-ba98-1ede54d1be19))
  (pad "" smd roundrect locked (at 0.42 -0.47) (size 0.7 0.79) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 171c1b40-57c3-4c79-9de1-3c136a15e253))
  (pad "" smd roundrect locked (at -0.42 0.47) (size 0.7 0.79) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 52b578cf-6d36-4228-97ea-30a9142656af))
  (pad "" smd roundrect locked (at 0.42 0.47) (size 0.7 0.79) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 66a8677a-23e7-407c-b464-21ad9b5a8f58))
  (pad "" smd roundrect locked (at -0.42 -0.47) (size 0.7 0.79) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp ff5b9009-661a-4621-96e6-d145b919fd36))
  (pad "1" smd roundrect locked (at -2.15 -1) (size 1.45 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 52a93e19-cc44-439d-92db-8af6ff5741fe))
  (pad "2" smd roundrect locked (at -2.15 -0.5) (size 1.45 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 59203bd7-88b4-4adb-97ea-dda269b68dbe))
  (pad "3" smd roundrect locked (at -2.15 0) (size 1.45 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c3c73602-b8a3-4da9-9910-1912dd70680b))
  (pad "4" smd roundrect locked (at -2.15 0.5) (size 1.45 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8e888504-e05f-4a0b-b10b-e8971bb49f3b))
  (pad "5" smd roundrect locked (at -2.15 1) (size 1.45 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4c6b04bd-3064-41ba-b588-82633160fc14))
  (pad "6" smd roundrect locked (at 2.15 1) (size 1.45 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 33919114-c3da-4a2d-9404-2f56f96362bc))
  (pad "7" smd roundrect locked (at 2.15 0.5) (size 1.45 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cef8b29f-26b3-434f-bdaa-ec7d9e290b4b))
  (pad "8" smd roundrect locked (at 2.15 0) (size 1.45 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 85d425e1-e6ce-4b04-b8ad-0a8133596a1f))
  (pad "9" smd roundrect locked (at 2.15 -0.5) (size 1.45 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 82c24d47-f743-44b0-b551-6ba4bcfb427f))
  (pad "10" smd roundrect locked (at 2.15 -1) (size 1.45 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4f94dc77-80d7-4f48-8228-9640c221dd50))
  (pad "11" thru_hole circle locked (at -0.55 -0.65) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 4e9cfc77-8b3a-4aed-abfb-ca8a21fb080b))
  (pad "11" smd rect locked (at 0 0) (size 1.68 1.88) (layers "F.Cu" "F.Mask") (tstamp 66123284-f549-46ca-9306-cb029bdc5041))
  (pad "11" smd rect locked (at 0 0) (size 1.6 1.8) (layers "B.Cu") (tstamp 823e043d-cedf-4b03-8ad1-05eaef967899))
  (pad "11" thru_hole circle locked (at -0.55 0.65) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp bdbe515a-cd73-434e-9445-406e317eaeec))
  (pad "11" thru_hole circle locked (at 0.55 0.65) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp edd1f3e2-4f3d-41ae-8916-d688b44e93e9))
  (pad "11" thru_hole circle locked (at 0.55 -0.65) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp fa9715f8-9eac-4a58-8a0b-77fda9d255bc))
  (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
