(footprint "QFN-48-1EP_7x7mm_P0.5mm_EP4.1x4.1mm_ThermalVias" (version 20210424) (generator pcbnew) (layer "F.Cu")
  (tedit 609DC66F)
  (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference "REF**" (at 0 -4.82) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 97107ec7-fa0d-468b-a766-8a7adcf27624)
  )
  (fp_text value "QFN-48-1EP_7x7mm_P0.5mm_EP4.1x4.1mm_ThermalVias" (at 0 4.82) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f8cef8ab-1649-49d4-9ad1-6efaaf4df093)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 378eb6ca-5716-4514-a961-91911086e3a7)
  )
  (fp_line (start -3.135 -3.61) (end -3.61 -3.61) (layer "F.SilkS") (width 0.12) (tstamp 04055922-a81f-40a5-9496-34d07cd50199))
  (fp_line (start 3.135 -3.61) (end 3.61 -3.61) (layer "F.SilkS") (width 0.12) (tstamp 2328fb11-686e-4e0d-ad16-a109e42657f5))
  (fp_line (start 3.61 3.61) (end 3.61 3.135) (layer "F.SilkS") (width 0.12) (tstamp 3764b29a-70fe-45de-9f57-abbfdab5157d))
  (fp_line (start 3.135 3.61) (end 3.61 3.61) (layer "F.SilkS") (width 0.12) (tstamp 3e4178de-e2b3-4ed5-8099-79c5393fd4b2))
  (fp_line (start -3.135 3.61) (end -3.61 3.61) (layer "F.SilkS") (width 0.12) (tstamp 4a79657e-6799-4b0f-926f-d7d82580812f))
  (fp_line (start 3.61 -3.61) (end 3.61 -3.135) (layer "F.SilkS") (width 0.12) (tstamp 643e0713-fd21-452c-bf57-2f77c2854a08))
  (fp_line (start -3.61 3.61) (end -3.61 3.135) (layer "F.SilkS") (width 0.12) (tstamp 92b2d90c-20c3-4399-9e3c-7a4536aa0e2e))
  (fp_line (start -4.12 4.12) (end 4.12 4.12) (layer "F.CrtYd") (width 0.05) (tstamp 1b1c7c83-f5a5-4d6e-ae44-347e28257dd2))
  (fp_line (start 4.12 4.12) (end 4.12 -4.12) (layer "F.CrtYd") (width 0.05) (tstamp 1e5d8215-18dc-4644-9505-394a247ac0f1))
  (fp_line (start -4.12 -4.12) (end -4.12 4.12) (layer "F.CrtYd") (width 0.05) (tstamp 3002406f-3242-4934-acc2-1093eb12ffa0))
  (fp_line (start 4.12 -4.12) (end -4.12 -4.12) (layer "F.CrtYd") (width 0.05) (tstamp fb5f73cf-45eb-4489-b2cc-3ff4c4a0c971))
  (fp_line (start -3.5 -2.5) (end -2.5 -3.5) (layer "F.Fab") (width 0.1) (tstamp 65b7447b-0b98-4ac2-a183-2923e7ec446a))
  (fp_line (start 3.5 -3.5) (end 3.5 3.5) (layer "F.Fab") (width 0.1) (tstamp 7f0a9af8-59e4-456c-8603-154018e68d3a))
  (fp_line (start -3.5 3.5) (end -3.5 -2.5) (layer "F.Fab") (width 0.1) (tstamp c215cfc0-6b91-487a-881e-41ff058a1920))
  (fp_line (start -2.5 -3.5) (end 3.5 -3.5) (layer "F.Fab") (width 0.1) (tstamp cca53863-a8c4-4976-ad84-94f9e19ac6e3))
  (fp_line (start 3.5 3.5) (end -3.5 3.5) (layer "F.Fab") (width 0.1) (tstamp db74aea6-4c35-4251-b124-c893436a868f))
  (pad "" smd roundrect locked (at -1.1625 -0.0125) (size 0.997293 0.997293) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 14d3979e-b869-4cf0-9ed8-8df9ff4b73de))
  (pad "" smd roundrect locked (at 1.1625 1.15) (size 0.997293 0.997293) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 29e42857-4ecd-4cd5-af9f-a903e29c31f9))
  (pad "" smd roundrect locked (at 1.1625 -0.0125) (size 0.997293 0.997293) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 30cfe023-4564-44b3-966a-ef603483a86e))
  (pad "" smd roundrect locked (at -1.1625 1.15) (size 0.997293 0.997293) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 4d956a8b-19ff-47b8-a2a0-796b80f91ee1))
  (pad "" smd roundrect locked (at 1.1625 -1.175) (size 0.997293 0.997293) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 6565af6c-2071-4a29-a51c-54f0128950b8))
  (pad "" smd roundrect locked (at 0 1.15) (size 0.997293 0.997293) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp a3d63cc3-069e-491c-910e-002b22894634))
  (pad "" smd roundrect locked (at 0 -0.0125) (size 0.997293 0.997293) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp b6227837-0f73-421d-ba64-f130a0d51030))
  (pad "" smd roundrect locked (at -1.1625 -1.175) (size 0.997293 0.997293) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp dfc9ca6b-b734-4e0a-a801-8fc8d356cf26))
  (pad "" smd roundrect locked (at 0 -1.175) (size 0.997293 0.997293) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp f97a34b1-77fa-4b44-a658-df203be58a17))
  (pad "1" smd roundrect locked (at -3.4375 -2.75) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 03c1e7df-3623-4db5-ad7a-c8a5e46a852e))
  (pad "2" smd roundrect locked (at -3.4375 -2.25) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fbfe4cb4-58ba-4ae4-80e8-858535b1e8ec))
  (pad "3" smd roundrect locked (at -3.4375 -1.75) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9c5b575e-ef6b-4000-8d54-82d514a45ecc))
  (pad "4" smd roundrect locked (at -3.4375 -1.25) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a14a51ce-9ebd-4899-9958-7cbe1dbdadef))
  (pad "5" smd roundrect locked (at -3.4375 -0.75) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9dda3919-0d7c-4849-b1b1-9a8db3b9ad48))
  (pad "6" smd roundrect locked (at -3.4375 -0.25) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 78ed8279-5181-4580-9396-f785b9602d80))
  (pad "7" smd roundrect locked (at -3.4375 0.25) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c319266d-15f3-474b-b824-7cd80eed0549))
  (pad "8" smd roundrect locked (at -3.4375 0.75) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d1fa2251-5796-4204-bb4c-50364bfeba84))
  (pad "9" smd roundrect locked (at -3.4375 1.25) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c0b5f0e0-af46-42c0-9310-33288be2db97))
  (pad "10" smd roundrect locked (at -3.4375 1.75) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9f728940-d443-4251-a207-8e0a199463d6))
  (pad "11" smd roundrect locked (at -3.4375 2.25) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 92825f33-9ca7-4945-8232-af22ef84e4cb))
  (pad "12" smd roundrect locked (at -3.4375 2.75) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 196f6bd4-e132-42dd-bcb1-08545fa01ee5))
  (pad "13" smd roundrect locked (at -2.75 3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d1037da6-487d-4eb2-bbe3-98386095db59))
  (pad "14" smd roundrect locked (at -2.25 3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bc5a6f20-a403-46b8-90dd-1d4c2e326f9e))
  (pad "15" smd roundrect locked (at -1.75 3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 158112d6-788a-4de2-957f-fc4288e6f81b))
  (pad "16" smd roundrect locked (at -1.25 3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5cb4f17c-0d31-44f5-9874-be1f170d1b5f))
  (pad "17" smd roundrect locked (at -0.75 3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 95da869c-c653-4fd8-b704-2dd1b89cbe14))
  (pad "18" smd roundrect locked (at -0.25 3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 769742f2-41a2-44f1-b3de-3658652541dd))
  (pad "19" smd roundrect locked (at 0.25 3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7732763e-2750-45e4-92d5-86acd3af7847))
  (pad "20" smd roundrect locked (at 0.75 3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5c019f3a-6e58-4138-af6a-67dbcdcddeaa))
  (pad "21" smd roundrect locked (at 1.25 3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e230b473-c42d-4b14-84fa-fb81f189d9e3))
  (pad "22" smd roundrect locked (at 1.75 3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 693c28b2-6e75-456e-8c23-2272e373cb58))
  (pad "23" smd roundrect locked (at 2.25 3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 97d5bcc7-f16b-495f-b8f8-b9a0586c9a02))
  (pad "24" smd roundrect locked (at 2.75 3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 429452d4-e545-456d-8200-971d9b24eb46))
  (pad "25" smd roundrect locked (at 3.4375 2.75) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b3230ba8-0c48-427c-8b5b-0c9179abc131))
  (pad "26" smd roundrect locked (at 3.4375 2.25) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 021a6cae-ea4d-42f2-974c-45427bf22940))
  (pad "27" smd roundrect locked (at 3.4375 1.75) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7334ba9c-86d4-4b9c-872e-a59f9b384d1a))
  (pad "28" smd roundrect locked (at 3.4375 1.25) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 77f431ed-94ee-4f28-821d-96ef8608604c))
  (pad "29" smd roundrect locked (at 3.4375 0.75) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp da98f516-9a31-45df-9e1d-d2bb75ff5ab6))
  (pad "30" smd roundrect locked (at 3.4375 0.25) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fa205e1f-02c9-486a-8cae-0f549fcf2911))
  (pad "31" smd roundrect locked (at 3.4375 -0.25) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 07bab4d5-bb20-4f0b-b667-1a474c09039d))
  (pad "32" smd roundrect locked (at 3.4375 -0.75) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9a121834-f74e-4322-a388-b89600ecfce7))
  (pad "33" smd roundrect locked (at 3.4375 -1.25) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2959bf71-5b1d-4f7f-9e41-b9b037254e9e))
  (pad "34" smd roundrect locked (at 3.4375 -1.75) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2c118507-c4f1-4a1c-b58a-65b3f114c7ca))
  (pad "35" smd roundrect locked (at 3.4375 -2.25) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 81a813fe-56b2-40be-a25e-47ea60ec8285))
  (pad "36" smd roundrect locked (at 3.4375 -2.75) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1a28215e-1f87-44de-ae1f-22b9d2d242d4))
  (pad "37" smd roundrect locked (at 2.75 -3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a7e46ed4-9a51-4064-94e0-73d3ea75e6f2))
  (pad "38" smd roundrect locked (at 2.25 -3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 31a973f1-fa1e-40df-b050-e20676f3706a))
  (pad "39" smd roundrect locked (at 1.75 -3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 822932c0-81f6-47ec-a4a1-3f1471c51355))
  (pad "40" smd roundrect locked (at 1.25 -3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1bf3d312-26f4-4cd9-93b8-a2134f930a32))
  (pad "41" smd roundrect locked (at 0.75 -3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ed2bde6c-c0d9-4cf0-89aa-badb63955581))
  (pad "42" smd roundrect locked (at 0.25 -3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1419755b-7ae1-40f4-b690-e885b76623b7))
  (pad "43" smd roundrect locked (at -0.25 -3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 00fdbb0e-ae08-4970-aba2-9fb910ba893c))
  (pad "44" smd roundrect locked (at -0.75 -3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f06b5803-2550-4011-9653-e408d9b18ff1))
  (pad "45" smd roundrect locked (at -1.25 -3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c9708781-86ec-4847-a95e-38adda35a29c))
  (pad "46" smd roundrect locked (at -1.75 -3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 377a029c-f848-46bf-a900-22f44688cbca))
  (pad "47" smd roundrect locked (at -2.25 -3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 122b3bc2-f179-49a4-af72-818c33923f7a))
  (pad "48" smd roundrect locked (at -2.75 -3.4375) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 22849cd0-1535-4b96-8d26-1e1b92fad64a))
  (pad "49" smd rect locked (at 0 0) (size 4.1 4.1) (layers "B.Cu") (tstamp 0d4c92bf-2099-44f5-8614-36cd57e6f47e))
  (pad "49" thru_hole circle locked (at 1.74375 0.56875) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 1ea23270-4d88-4414-9493-a5e24cd00a7e))
  (pad "49" thru_hole circle locked (at -1.74375 -0.59375) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 20b3cbd7-3ce4-4047-b5a6-cdc78f617029))
  (pad "49" smd rect locked (at 0 0) (size 4.1 4.1) (layers "F.Cu" "F.Mask") (tstamp 235271d2-0788-4b21-ba26-5d0715b43757))
  (pad "49" thru_hole circle locked (at 0.58125 1.73125) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 23d1e049-7e54-4f52-a0f9-7725dc971695))
  (pad "49" thru_hole circle locked (at 0.58125 -1.75) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 31477f4a-891f-453f-9228-ef8a3e216172))
  (pad "49" thru_hole circle locked (at -1.74375 0.56875) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 80eb9fbe-42eb-4aa3-968a-1b01fd5d3673))
  (pad "49" thru_hole circle locked (at -0.58125 -1.75) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp 9316243d-b0b1-49f6-8e34-a6f8940c8866))
  (pad "49" thru_hole circle locked (at 1.74375 -0.59375) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp a3a717ed-30db-41f6-bd32-f400e71cb90c))
  (pad "49" thru_hole circle locked (at 0.58125 -0.59375) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp b481477d-535f-4190-9374-a69d525347f3))
  (pad "49" thru_hole circle locked (at -0.58125 -0.59375) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp c800ef8e-5a46-43e0-a31c-5293b2083eea))
  (pad "49" thru_hole circle locked (at -0.58125 0.56875) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp d9e8a846-61d3-4573-a122-34288a77fbed))
  (pad "49" thru_hole circle locked (at -0.58125 1.73125) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp ee2ef68f-de3c-4526-bdf1-482fd873e4bb))
  (pad "49" thru_hole circle locked (at 0.58125 0.56875) (size 0.6 0.6) (drill 0.3) (layers *.Cu) (tstamp f00b1dbd-a2d0-4187-8a1d-92bb27c0d2e4))
  (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
