(footprint "MPS_QFN-16_3x3mm_P0.4mm" (version 20210824) (generator pcbnew) (layer "F.Cu")
  (tedit 617DE2D1)
  (descr "QFN, 16 Pin (https://www.onsemi.com/pub/Collateral/NCN4555-D.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.8) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 253ad3be-bbf2-4649-a1b3-644fe5eadd25)
  )
  (fp_text value "MPS_QFN-16_3x3mm_P0.4mm" (at 0 2.8) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3ca4b86c-153d-406a-a8f5-5a5c8e44c32d)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 0.75 0.75) (thickness 0.11)))
    (tstamp 25deccaf-e248-4811-aebc-6567f66a5e62)
  )
  (fp_line (start -1.135 1.61) (end -1.61 1.61) (layer "F.SilkS") (width 0.12) (tstamp 4373d0c4-b3b5-4132-9122-8fe1d8f8ed3f))
  (fp_line (start -1.135 -1.61) (end -1.61 -1.61) (layer "F.SilkS") (width 0.12) (tstamp 6f36dca7-8f7b-4455-be4c-08e8c3496f57))
  (fp_line (start -1.61 1.61) (end -1.61 1.135) (layer "F.SilkS") (width 0.12) (tstamp b777386f-c001-461a-9408-22439c3bafbf))
  (fp_line (start 1.135 1.61) (end 1.61 1.61) (layer "F.SilkS") (width 0.12) (tstamp cc60050b-0a50-4e2f-9068-ea4844a36683))
  (fp_line (start 1.61 -1.61) (end 1.61 -1.135) (layer "F.SilkS") (width 0.12) (tstamp de785984-1b6a-4a64-9491-8dfcf4394b2d))
  (fp_line (start 1.135 -1.61) (end 1.61 -1.61) (layer "F.SilkS") (width 0.12) (tstamp ed5eb809-2d80-41eb-a54a-9fd6c64c8ad9))
  (fp_line (start 1.61 1.61) (end 1.61 1.135) (layer "F.SilkS") (width 0.12) (tstamp fe2bda4b-b0bc-4957-be19-d3628817ba5f))
  (fp_line (start -2.1 2.1) (end 2.1 2.1) (layer "F.CrtYd") (width 0.05) (tstamp 3055c6d2-11ab-4c21-8ee6-d5cf7a42c4d1))
  (fp_line (start 2.1 2.1) (end 2.1 -2.1) (layer "F.CrtYd") (width 0.05) (tstamp 55418d6f-b416-4c9b-8990-f29f886f9d97))
  (fp_line (start 2.1 -2.1) (end -2.1 -2.1) (layer "F.CrtYd") (width 0.05) (tstamp 8169906b-1ece-4b6a-807f-34ed67b5940c))
  (fp_line (start -2.1 -2.1) (end -2.1 2.1) (layer "F.CrtYd") (width 0.05) (tstamp 98eb6a45-53e4-4caf-8833-d774754d615a))
  (fp_line (start -1.5 1.5) (end -1.5 -0.75) (layer "F.Fab") (width 0.1) (tstamp 422911c8-b128-479c-8a10-9491579bc341))
  (fp_line (start -1.5 -0.75) (end -0.75 -1.5) (layer "F.Fab") (width 0.1) (tstamp 79f9ca4a-a7f5-4a52-abd8-322e3b605bce))
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer "F.Fab") (width 0.1) (tstamp d1a3b0a2-7a53-4649-b90a-8bf4ad23208b))
  (fp_line (start -0.75 -1.5) (end 1.5 -1.5) (layer "F.Fab") (width 0.1) (tstamp e7d51db2-35bb-49be-a2fc-8ade3661697a))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer "F.Fab") (width 0.1) (tstamp f33de0da-c341-4a94-b1db-db046a5af863))
  (pad "1" smd roundrect locked (at -1.25 -0.525) (size 1.1 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 385d3ca5-b567-470d-914f-ddd7632854c8))
  (pad "2" smd roundrect locked (at -1.25 0.175) (size 1.1 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9011b3a7-4e96-43c6-913c-77f48379576b))
  (pad "3" smd roundrect locked (at -0.8 1.45 90) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d2c205a3-b477-4c54-8d39-23f44469a659))
  (pad "4" smd roundrect locked (at -0.4 1.45 90) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6764ba50-c511-45e7-bc60-8b756e561fd8))
  (pad "5" smd roundrect locked (at 0 1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f1068a3d-d1e6-4414-9786-e06c3c4390b6))
  (pad "6" smd roundrect locked (at 0.4 1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c88b2b14-624b-4172-a286-7a0c4c6846a1))
  (pad "7" smd roundrect locked (at 0.8 1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b5e45bfd-14e3-436b-bbe0-1dee30e79622))
  (pad "8" smd roundrect locked (at 1.25 0.525 90) (size 0.2 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 91810cf8-cf0c-4b64-a029-cea848a0764d))
  (pad "9" smd roundrect locked (at 1.25 -0.175) (size 1.1 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 62072be9-1d34-486a-84af-50ca56ca6fae))
  (pad "10" smd roundrect locked (at 0.8 -1.45 90) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b5e6b0b6-ea2c-4d10-827c-d9986efb521d))
  (pad "11" smd roundrect locked (at 0.4 -1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ff493ba9-fb1c-41b5-b564-55a403f30390))
  (pad "12" smd roundrect locked (at 0 -1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 01931c51-c523-4668-8233-8e48dab6969a))
  (pad "13" smd roundrect locked (at -0.4 -1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5b11ed48-d62b-458a-9e37-1e5a46460d9f))
  (pad "14" smd roundrect locked (at -0.8 -1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 441626a6-2b4e-4624-8468-6def372d2b8e))
  (pad "15" smd roundrect locked (at 0 -0.165) (size 0.65 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1069d234-0fe7-4378-8656-6ec3a463e939))
  (pad "16" smd roundrect locked (at 0 0.435) (size 0.65 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 94788306-ac9d-4d4a-8ff0-b4b04419132e))
  (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
