From 727e4b1a1d921520b5b5dc08869eb12b11ba248f Mon Sep 17 00:00:00 2001
From: Sergey Larin <cerg2010cerg2010@mail.ru>
Date: Sun, 10 Feb 2019 00:43:16 +0300
Subject: [PATCH] ARM: dts: tegra20-glide: fix AK8975

Add GPIO definition instead of interrupt.

Signed-off-by: Sergey Larin <cerg2010cerg2010@mail.ru>
---
 arch/arm/boot/dts/tegra20-glide.dts | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

diff --git a/arch/arm/boot/dts/tegra20-glide.dts b/arch/arm/boot/dts/tegra20-glide.dts
index 87d737c62b0a..f1909f55d8e3 100644
--- a/arch/arm/boot/dts/tegra20-glide.dts
+++ b/arch/arm/boot/dts/tegra20-glide.dts
@@ -835,8 +835,7 @@
 		ak8975@c {
 			compatible = "asahi-kasei,ak8975";
 			reg = <0xc>;
-			interrupt-parent = <&gpio>;
-			interrupts = <TEGRA_GPIO(K, 4) IRQ_TYPE_LEVEL_HIGH>;
+			gpios = <&gpio TEGRA_GPIO(K, 4) GPIO_ACTIVE_HIGH>;
 		};
 	};
 
-- 
2.22.0

