# Reference: <https://postmarketos.org/devicepkg>
pkgname=device-pine64-a64lts
pkgdesc="PINE64 A64-LTS"
pkgver=1
pkgrel=1
url="https://postmarketos.org"
license="MIT"
arch="aarch64"
options="!check !archcheck"
subpackages="$pkgname-nonfree-firmware:nonfree_firmware"
depends="postmarketos-base linux-postmarketos-allwinner u-boot-sunxi u-boot-tools"
makedepends="devicepkg-dev"
source="
	deviceinfo
	uboot-script.cmd
"

build() {
	devicepkg_build $startdir $pkgname
	mkimage -A arm -O linux -T script -C none -a 0 -e 0 -n postmarketos -d "$srcdir"/uboot-script.cmd "$srcdir"/boot.scr
}

package() {
	devicepkg_package $startdir $pkgname
	install -D -m644 "$srcdir"/boot.scr \
		"$pkgdir"/boot/boot.scr
}

nonfree_firmware() {
	pkgdesc="Wifi and Bluetooth firmware"
	depends="linux-firmware-rtlwifi linux-firmware-rtl_bt firmware-pine64-rtl8723bt"
	mkdir "$subpkgdir"
}

sha512sums="
b6fe933886888b453839084d2001de93f343472d1f4e2597914901692d9410d15202f790d92a3f70312e4ededd687f02edd79423ea7b9a9f831f6db57f9093fa  deviceinfo
9f53b80ebc9cbbea488c75dc9b3abe374d5a5e6b756831dd5d298fd4af73450fedea5cc93381f93bbbdd3503cffd4ea5edb2a6836ea130fb408327ea4cf12576  uboot-script.cmd
"
