From aa5360534ba836cb5cee6a574c6aec2666ce2b3a Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Filip=20Matijevi=C4=87?= <filip.matijevic.pz@gmail.com>
Date: Wed, 1 Nov 2017 18:25:45 +0100
Subject: [PATCH 06/11] HACK: drm/omap: panel-dsi-cm: force 0xff for brigthness
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Filip Matijević <filip.matijevic.pz@gmail.com>
---
 drivers/gpu/drm/omapdrm/displays/panel-dsi-cm.c | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/drivers/gpu/drm/omapdrm/displays/panel-dsi-cm.c b/drivers/gpu/drm/omapdrm/displays/panel-dsi-cm.c
index 09ddbb001123..b77e4925941a 100644
--- a/drivers/gpu/drm/omapdrm/displays/panel-dsi-cm.c
+++ b/drivers/gpu/drm/omapdrm/displays/panel-dsi-cm.c
@@ -375,6 +375,8 @@ static int dsicm_bl_update_status(struct backlight_device *dev)
 	else
 		level = 0;
 
+	level = 0xff;
+
 	dev_dbg(&ddata->pdev->dev, "update brightness to %d\n", level);
 
 	mutex_lock(&ddata->lock);
-- 
2.17.0

