#!/bin/sh

# When device is finished booting, stop the default boot animation and replace it with a rainbow
echo 0 > /sys/bus/i2c/devices/0-003f/boot_animation
echo "0000ff0000ff4f00cf4f00cfff0000ff0000af2f00af2f00ffff00ffff0000ff0000ff00" > /sys/bus/i2c/devices/0-003f/frame
