diff --git a/arch/arm64/boot/dts/qcom/Makefile b/arch/arm64/boot/dts/qcom/Makefile
index 39889d5f8..019d7a157 100644
--- a/arch/arm64/boot/dts/qcom/Makefile
+++ b/arch/arm64/boot/dts/qcom/Makefile
@@ -58,6 +58,7 @@ dtb-$(CONFIG_ARCH_QCOM)	+= msm8956-sony-xperia-loire-kugo.dtb
 dtb-$(CONFIG_ARCH_QCOM)	+= msm8956-sony-xperia-loire-suzu.dtb
 dtb-$(CONFIG_ARCH_QCOM)	+= msm8992-lg-bullhead-rev-10.dtb
 dtb-$(CONFIG_ARCH_QCOM)	+= msm8992-lg-bullhead-rev-101.dtb
+dtb-$(CONFIG_ARCH_QCOM)	+= msm8992-lg-h815.dtb
 dtb-$(CONFIG_ARCH_QCOM)	+= msm8992-msft-lumia-octagon-talkman.dtb
 dtb-$(CONFIG_ARCH_QCOM)	+= msm8992-xiaomi-libra.dtb
 dtb-$(CONFIG_ARCH_QCOM)	+= msm8994-huawei-angler-rev-101.dtb
diff --git a/arch/arm64/boot/dts/qcom/msm8992-lg-h815.dts b/arch/arm64/boot/dts/qcom/msm8992-lg-h815.dts
new file mode 100644
index 000000000..6767e9be1
--- /dev/null
+++ b/arch/arm64/boot/dts/qcom/msm8992-lg-h815.dts
@@ -0,0 +1,386 @@
+// SPDX-License-Identifier: GPL-2.0-only
+
+/dts-v1/;
+
+#include "msm8992.dtsi"
+#include "pm8994.dtsi"
+#include "pmi8994.dtsi"
+
+/delete-node/ &cont_splash_mem;
+
+/* disabled downstream */
+/delete-node/ &dfps_data_mem;
+
+/ {
+	model = "LG G4 (H815)";
+	compatible = "lg,h815", "qcom,msm8992";
+	chassis-type = "handset";
+
+	/* required for bootloader to select correct board */
+	qcom,msm-id = <251 0 252 0>;
+	qcom,pmic-id = <0x10009 0x1000a 0x00 0x00>;
+	qcom,board-id = <0xb64 0>;
+
+	/* psci is broken */
+	/delete-node/ psci;
+
+	chosen {};
+
+	gpio-hall-sensor {
+		compatible = "gpio-keys";
+
+		pinctrl-0 = <&hall_sensor_default>;
+		pinctrl-names = "default";
+
+		event-hall-sensor {
+			gpios = <&tlmm 75 GPIO_ACTIVE_LOW>;
+			label = "hall effect sensor";
+			linux,input-type = <EV_SW>;
+			linux,code = <SW_LID>;
+			linux,can-disable;
+			wakeup-source;
+		};
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		autorepeat;
+
+		key-vol-up {
+			label = "volume up";
+			gpios = <&pm8994_gpios 3 GPIO_ACTIVE_LOW>;
+			linux,code = <KEY_VOLUMEUP>;
+			wakeup-source;
+			debounce-interval = <15>;
+		};
+	};
+
+	reserved-memory {
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+
+		ramoops@ff00000 {
+			compatible = "ramoops";
+			reg = <0x0 0xff00000 0x0 0x100000>;
+			console-size = <0x20000>;
+			pmsg-size = <0x20000>;
+			record-size = <0x10000>;
+			ecc-size = <0x10>;
+		};
+
+		cont_splash_mem: fb@3400000 {
+			compatible = "framebuffer";
+			reg = <0 0x3400000 0 0xc00000>;
+			no-map;
+		};
+
+		crash_fb_mem: crash_fb@4000000 {
+			reg = <0 0x4000000 0 0xc00000>;
+			no-map;
+		};
+	};
+};
+
+&pm8994_spmi_regulators {
+	vdd_s8-supply = <&vph_pwr>;
+	vdd_s11-supply = <&vph_pwr>;
+
+	pm8994_s8: s8 {
+		regulator-min-microvolt = <700000>;
+		regulator-max-microvolt = <1180000>;
+		regulator-always-on;
+		regulator-boot-on;
+	};
+
+	pm8994_s11: s11 {
+		regulator-min-microvolt = <700000>;
+		regulator-max-microvolt = <1225000>;
+		regulator-always-on;
+		regulator-boot-on;
+	};
+};
+
+&rpm_requests {
+	pmi8994_regulators: pmi8994-regulators {
+		compatible = "qcom,rpm-pmi8994-regulators";
+
+		vdd_s1-supply = <&vph_pwr>;
+		vdd_bst_byp-supply = <&vph_pwr>;
+
+		pmi8994_s1: s1 {
+			regulator-min-microvolt = <1025000>;
+			regulator-max-microvolt = <1025000>;
+		};
+
+		/* S2 & S3 - VDD_GFX */
+
+		pmi8994_bby: boost-bypass {
+			regulator-min-microvolt = <3150000>;
+			regulator-max-microvolt = <3600000>;
+		};
+	};
+
+	pm8994_regulators: pm8994-regulators {
+		compatible = "qcom,rpm-pm8994-regulators";
+
+		vdd_s3-supply = <&vph_pwr>;
+		vdd_s4-supply = <&vph_pwr>;
+		vdd_s5-supply = <&vph_pwr>;
+		vdd_s7-supply = <&vph_pwr>;
+		vdd_l1-supply = <&pmi8994_s1>;
+		vdd_l2_26_28-supply = <&pm8994_s3>;
+		vdd_l3_11-supply = <&pm8994_s3>;
+		vdd_l4_27_31-supply = <&pm8994_s3>;
+		vdd_l5_7-supply = <&pm8994_s5>;
+		vdd_l6_12_32-supply = <&pm8994_s5>;
+		vdd_l8_16_30-supply = <&vph_pwr>;
+		vdd_l9_10_18_22-supply = <&pmi8994_bby>;
+		vdd_l13_19_23_24-supply = <&pmi8994_bby>;
+		vdd_l14_15-supply = <&pm8994_s5>;
+		vdd_l17_29-supply = <&pmi8994_bby>;
+		vdd_l20_21-supply = <&pmi8994_bby>;
+		vdd_l25-supply = <&pm8994_s5>;
+		vdd_lvs1_2 = <&pm8994_s4>;
+
+		pm8994_s3: s3 {
+			regulator-min-microvolt = <1300000>;
+			regulator-max-microvolt = <1300000>;
+		};
+
+		/* sdhc1 vqmmc and bcm */
+		pm8994_s4: s4 {
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+			regulator-system-load = <325000>;
+			regulator-allow-set-load;
+		};
+
+		pm8994_s5: s5 {
+			regulator-min-microvolt = <2150000>;
+			regulator-max-microvolt = <2150000>;
+		};
+
+		pm8994_s7: s7 {
+			regulator-min-microvolt = <1000000>;
+			regulator-max-microvolt = <1000000>;
+		};
+
+		pm8994_l1: l1 {
+			regulator-min-microvolt = <1000000>;
+			regulator-max-microvolt = <1000000>;
+		};
+
+		pm8994_l2: l2 {
+			regulator-min-microvolt = <1250000>;
+			regulator-max-microvolt = <1250000>;
+			regulator-system-load = <10000>;
+			regulator-allow-set-load;
+		};
+
+		/* camera */
+		pm8994_l3: l3 {
+			regulator-min-microvolt = <1050000>;
+			regulator-max-microvolt = <1050000>;
+		};
+
+		pm8994_l4: l4 {
+			regulator-min-microvolt = <1225000>;
+			regulator-max-microvolt = <1225000>;
+		};
+
+		/* L5 is inaccessible from RPM */
+
+		pm8994_l6: l6 {
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+		};
+
+		/* L7 is inaccessible from RPM */
+
+		pm8994_l8: l8 {
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+		};
+
+		pm8994_l9: l9 {
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+		};
+
+		/* touch  */
+		pm8994_l10: l10 {
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+		};
+
+		pm8994_l11: l11 {
+			regulator-min-microvolt = <1200000>;
+			regulator-max-microvolt = <1200000>;
+		};
+
+		pm8994_l12: l12 {
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+			regulator-system-load = <10000>;
+			regulator-allow-set-load;
+		};
+
+		/* sdhc2 vqmmc */
+		pm8994_l13: l13 {
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <2950000>;
+			regulator-system-load = <22000>;
+			regulator-allow-set-load;
+		};
+
+		/* camera */
+		pm8994_l14: l14 {
+			regulator-min-microvolt = <1200000>;
+			regulator-max-microvolt = <1200000>;
+			regulator-system-load = <10000>;
+			regulator-allow-set-load;
+		};
+
+		pm8994_l15: l15 {
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+		};
+
+		pm8994_l16: l16 {
+			regulator-min-microvolt = <2700000>;
+			regulator-max-microvolt = <2700000>;
+		};
+
+		/* camera */
+		pm8994_l17: l17 {
+			regulator-min-microvolt = <2800000>;
+			regulator-max-microvolt = <2800000>;
+		};
+
+		pm8994_l18: l18 {
+			regulator-min-microvolt = <2850000>;
+			regulator-max-microvolt = <2850000>;
+		};
+
+		/* LCD */
+		pm8994_l19: l19 {
+			regulator-min-microvolt = <3000000>;
+			regulator-max-microvolt = <3000000>;
+		};
+
+		/* sdhc1 vmmc */
+		pm8994_l20: l20 {
+			regulator-min-microvolt = <2950000>;
+			regulator-max-microvolt = <2950000>;
+			regulator-system-load = <570000>;
+			regulator-allow-set-load;
+		};
+
+		/* sdhc2 vmmc */
+		pm8994_l21: l21 {
+			regulator-min-microvolt = <2950000>;
+			regulator-max-microvolt = <2950000>;
+			regulator-system-load = <800000>;
+			regulator-allow-set-load;
+		};
+
+		/* touch */
+		pm8994_l22: l22 {
+			regulator-min-microvolt = <3000000>;
+			regulator-max-microvolt = <3000000>;
+		};
+
+		/* camera */
+		pm8994_l23: l23 {
+			regulator-min-microvolt = <2800000>;
+			regulator-max-microvolt = <2800000>;
+		};
+
+		pm8994_l24: l24 {
+			regulator-min-microvolt = <3075000>;
+			regulator-max-microvolt = <3150000>;
+		};
+
+		/* IRRC */
+		pm8994_l25: l25 {
+			regulator-min-microvolt = <1000000>;
+			regulator-max-microvolt = <1000000>;
+		};
+
+		pm8994_l26: l26 {
+			regulator-min-microvolt = <987500>;
+			regulator-max-microvolt = <987500>;
+		};
+
+		/* hdmi */
+		pm8994_l27: l27 {
+			regulator-min-microvolt = <1000000>;
+			regulator-max-microvolt = <1000000>;
+		};
+
+		pm8994_l28: l28 {
+			regulator-min-microvolt = <1000000>;
+			regulator-max-microvolt = <1000000>;
+			regulator-system-load = <10000>;
+			regulator-allow-set-load;
+		};
+
+		/* camera */
+		pm8994_l29: l29 {
+			regulator-min-microvolt = <2800000>;
+			regulator-max-microvolt = <2800000>;
+		};
+
+		/* camera */
+		pm8994_l30: l30 {
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+		};
+
+		pm8994_l31: l31 {
+			regulator-min-microvolt = <1262500>;
+			regulator-max-microvolt = <1262500>;
+		};
+
+		pm8994_l32: l32 {
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+		};
+
+		pm8994_lvs1: lvs1 {};
+
+		pm8994_lvs2: lvs2 {};
+	};
+};
+
+&pm8994_pon {
+	resin {
+		status = "okay";
+		linux,code = <KEY_VOLUMEDOWN>;
+	};
+};
+
+&tlmm {
+	hall_sensor_default: hall-sensor-default-state {
+		pins = "gpio75";
+		function = "gpio";
+		drive-strength = <2>;
+		bias-pull-up;
+	};
+};
+
+&sdhc1 {
+	status = "okay";
+	mmc-hs400-1_8v;
+	vmmc-supply = <&pm8994_l20>;
+	vqmmc-supply = <&pm8994_s4>;
+	non-removable;
+};
+
+&sdhc2 {
+	status = "okay";
+	vmmc-supply = <&pm8994_l21>;
+	vqmmc-supply = <&pm8994_l13>;
+	cd-gpios = <&pm8994_gpios 8 GPIO_ACTIVE_LOW>;
+};
