#!/sbin/openrc-run
supervisor=supervise-daemon

name="TA services"
description="TA services for msm8974-based Sony Xperia devices"

command="/usr/bin/ta-service"
command_args="/dev/disk/by-partlabel/TA"
