# Reference: <https://postmarketos.org/devicepkg>
# Maintainer: Nikita Travkin <nikita@trvn.ru>
pkgname=device-qcom-msm8916
pkgdesc="Generic device package for various Qualcomm MSM8916/MSM8939-based devices"
pkgver=2
pkgrel=1
url="https://postmarketos.org"
license="MIT"
arch="aarch64"
options="!check !archcheck"
depends="
	postmarketos-base
	soc-qcom-msm8916
"
makedepends="devicepkg-dev"
source="
	deviceinfo
	modules-initfs
"
subpackages="
	$pkgname-nonfree-firmware:nonfree_firmware
	$pkgname-kernel-extlinux:kernel_extlinux
	$pkgname-kernel-efi:kernel_efi
"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname
}

nonfree_firmware() {
	pkgdesc="WiFi/BT/Modem/Video firmware"
	depends="msm-firmware-loader firmware-qcom-adreno-a300 firmware-qcom-adreno-a420 firmware-qcom-db410c-wcnss-nv"
	mkdir "$subpkgdir"

	# HACK: For devices that don't have a nv file in persist we
	# temporarily link the db410c file to the expected location.
	# It will be overriden if the file is in persist or when user
	# installs the device-specific firmware packages.
	mkdir -p "$subpkgdir"/lib/firmware/wlan/prima/
	ln -s /lib/firmware/qcom/apq8016/WCNSS_qcom_wlan_nv_sbc.bin \
		"$subpkgdir"/lib/firmware/wlan/prima/WCNSS_qcom_wlan_nv.bin
}

kernel_extlinux() {
	pkgdesc="Use lk2nd to boot via extlinux.conf"
	depends="linux-postmarketos-qcom-msm8916"
	devicepkg_subpackage_kernel $startdir $pkgname $subpkgname
}

kernel_efi() {
	pkgdesc="Use U-Boot to boot via EFI"
	depends="linux-postmarketos-qcom-msm8916 systemd-boot"
	devicepkg_subpackage_kernel $startdir $pkgname $subpkgname
}

sha512sums="
0894e6a63f69062d4c9e744cdda700b30c68795fdfdc866b8c60c0d0d27b97f3ad915615d87baede2fdaceb5c2773240c649eb95d82b2d58acd5b59f1e5190c0  deviceinfo
80b037998756dab0c6b2a3bb438fb2d6bf727148c4af29648074b85c3beacdbbbffb2fefd477e68904d4c3bedb76bf0e532719a15a3bb7c8ef5f922be0d73c1d  modules-initfs
"
