From 18dfe3c57801796fb6ca2a17f63893e48298eaa4 Mon Sep 17 00:00:00 2001
From: David Wronek <davidwronek@gmail.com>
Date: Thu, 24 Aug 2023 11:15:05 +0200
Subject: [PATCH 5/8] arm64: dts: qcom: pm6150: Add resin and rtc nodes

Add support for the RTC which is the same as on other PMICs and add the
resin child node to the PM6150 PON device, both disabled by default.

Signed-off-by: David Wronek <davidwronek@gmail.com>
Tested-by: Nikita Travkin <nikita@trvn.ru>
Reviewed-by: Konrad Dybcio <konrad.dybcio@linaro.org>
Link: https://lore.kernel.org/r/20230824091737.75813-3-davidwronek@gmail.com
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
---
 arch/arm64/boot/dts/qcom/pm6150.dtsi | 16 ++++++++++++++++
 1 file changed, 16 insertions(+)

diff --git a/arch/arm64/boot/dts/qcom/pm6150.dtsi b/arch/arm64/boot/dts/qcom/pm6150.dtsi
index 7d4d1f2767ed..ddbaf7280b03 100644
--- a/arch/arm64/boot/dts/qcom/pm6150.dtsi
+++ b/arch/arm64/boot/dts/qcom/pm6150.dtsi
@@ -53,6 +53,14 @@ pm6150_pwrkey: pwrkey {
 				bias-pull-up;
 				linux,code = <KEY_POWER>;
 			};
+
+			pm6150_resin: resin {
+				compatible = "qcom,pm8941-resin";
+				interrupts = <0x0 0x8 1 IRQ_TYPE_EDGE_BOTH>;
+				debounce = <15625>;
+				bias-pull-up;
+				status = "disabled";
+			};
 		};
 
 		pm6150_temp: temp-alarm@2400 {
@@ -88,6 +96,14 @@ pm6150_adc_tm: adc-tm@3500 {
 			status = "disabled";
 		};
 
+		pm6150_rtc: rtc@6000 {
+			compatible = "qcom,pm8941-rtc";
+			reg = <0x6000>, <0x6100>;
+			reg-names = "rtc", "alarm";
+			interrupts = <0x0 0x61 0x1 IRQ_TYPE_EDGE_RISING>;
+			status = "disabled";
+		};
+
 		pm6150_gpios: gpio@c000 {
 			compatible = "qcom,pm6150-gpio", "qcom,spmi-gpio";
 			reg = <0xc000>;
-- 
2.43.2

