# Archived: Downstream port, only for testing. Use mainline port (samsung-m0/samsung-m3)!
# Reference: <https://postmarketos.org/devicepkg>
pkgname=device-samsung-m0-downstream
pkgdesc="Samsung Galaxy S III"
pkgver=3
pkgrel=4
url="https://postmarketos.org"
license="MIT"
arch="armv7"
options="!check !archcheck"
depends="
	linux-samsung-m0-downstream
	mkbootimg
	postmarketos-base
	postmarketos-initramfs-minimal
	"
makedepends="devicepkg-dev"
install="$pkgname.post-install"
subpackages="$pkgname-nonfree-firmware:nonfree_firmware"
source="
	deviceinfo
	90-android-touch-dev.rules
	"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname

	install -D -m644 "$srcdir"/90-android-touch-dev.rules \
		"$pkgdir"/etc/udev/rules.d/90-android-touch-dev.rules
}

nonfree_firmware() {
	pkgdesc="WiFi firmware"
	depends="firmware-samsung-m0-downstream"
	mkdir "$subpkgdir"
}

sha512sums="
e89b2287780aa94e93ee8cba472ec78b14a0de0089c3ee8c278175ace459d84a58a9278f473d917dd569b114874fb76931b404f810220d328c7e3f6148dac485  deviceinfo
1376f0eb7c6ba459ca5c44b3eb7e9919d9c5f48d71ec30c006d1b4843e31cdade9f980415a166e977b2567b26f4e87d4554ee1143fdc62453d60a93bed129d06  90-android-touch-dev.rules
"
