# Reference: <https://postmarketos.org/devicepkg>
# Unmaintained: no maintainer

pkgname=device-odroid-hc2
pkgdesc="ODROID HC2"
pkgver=1
pkgrel=1
url="https://postmarketos.org"
license="MIT"
arch="armv7"
options="!check !archcheck"
depends="linux-edge
	 postmarketos-base
	 u-boot-odroid
	 u-boot-tools
	"
makedepends="devicepkg-dev"
subpackages="$pkgname-nonfree-firmware:nonfree_firmware $pkgname-tools"
_commit="42ac93dcfbbb8a08c2bdc02e19f96eb35a81891a"
source="deviceinfo modules-initfs uboot-script.cmd install-rootfs-hdd.sh"

build() {
	devicepkg_build $startdir $pkgname
	mkimage \
		-A arm \
		-O linux \
		-T script \
		-C none \
		-a 0 \
		-e 0 \
		-n postmarketos \
		-d "$srcdir"/uboot-script.cmd \
		"$srcdir"/boot.scr
}

package() {
	devicepkg_package $startdir $pkgname
	install -Dm644 "$srcdir"/boot.scr \
		"$pkgdir"/boot/boot.scr
}

nonfree_firmware() {
	pkgdesc="U-Boot, Samsung JPEG encoder, and Realtek firmware, required for a bootable system"
	depends="firmware-odroid-hc2 linux-firmware-rtl_nic linux-firmware-other linux-firmware-s5p-mfc"
	mkdir "$subpkgdir"
}

tools() {
	pkgdesc="ODROID HC2 tools"
	depends="rsync e2fsprogs-extra"
	mkdir "$subpkgdir"
	install -Dm744 "$srcdir"/install-rootfs-hdd.sh \
		"$subpkgdir"/usr/bin/install-rootfs-hdd
}

sha512sums="
2aff998527535760d04b338d59976408a1d852ba38dfbdff305ec028030d419259cb1b9491b8e54a3621d147f9e8c1a797ed2a3784da7f25d2a92aa60882d027  deviceinfo
228726f7afca55b02e4d452904d8490cf15957edd59cc87274d89c8589f9d15044db87a4413053243e66aa1b22860cfda052b5b95395effaf3aaf4d1770d3fd3  modules-initfs
7e5056f648a81d0784b1b3a641e2f79c22d2b570c7f00092236b301b1545eefca3a6a353c1ad308114f66ac68481f1491df42ca5c6f8297c76e5ee0fa7af178f  uboot-script.cmd
09a2191dce5b5c8fdf80c4473d9773a51f2c633db51477f2f64983dd030d7800fd80999a228ec7efe3f9feafeba35902bff68cf95e6ae59048dc64424f402b63  install-rootfs-hdd.sh
"
