# Kernel config based on: arch/arm64/configs/ze550kl_defconfig

pkgname="linux-asus-z00t"
pkgver=3.10.108
pkgrel=2
pkgdesc="Zenfone 2 Laser/Selfie (1080p) kernel fork"
arch="aarch64"
_carch="arm64"
_flavor="asus-z00t"
url="https://kernel.org"
license="GPL2"
options="!strip !check !tracedeps"
makedepends="perl sed installkernel bash gmp-dev bc linux-headers elfutils-dev dtbtool gcc6"

# Compiler: this kernel was only tested with GCC6. Feel free to make a merge
# request if you find out that it is booting working with newer GCCs as
# well. See <https://postmarketos.org/vendorkernel> for instructions.
if [ "${CC:0:5}" != "gcc6-" ]; then
	CC="gcc6-$CC"
	HOSTCC="gcc6-gcc"
	CROSS_COMPILE="gcc6-$CROSS_COMPILE"
fi

# Source
_repository="android_kernel_asus_msm8916"
_commit="5fd66aa9219bf9aaa504aa3cb2dae7a3de5238f7"
_config="config-${_flavor}.${arch}"
source="
	$pkgname-$_commit.tar.gz::https://github.com/LineageOS/${_repository}/archive/${_commit}.tar.gz
	$_config
	compiler-gcc6.h
	01_fix_gcc6_errors.patch
	02_mdss_fb_refresh_rate.patch
	05_dtb-fix.patch
"
builddir="$srcdir/${_repository}-${_commit}"

prepare() {
	default_prepare

	# gcc6 support
	cp -v "$srcdir/compiler-gcc6.h" "$builddir/include/linux/"

	# Remove -Werror from all makefiles
	local i
	local makefiles="$(find . -type f -name Makefile)
		$(find . -type f -name Kbuild)"
	for i in $makefiles; do
		sed -i 's/-Werror-/-W/g' "$i"
		sed -i 's/-Werror//g' "$i"
	done

	# Prepare kernel config ('yes ""' for kernels lacking olddefconfig)
	cp "$srcdir"/$_config "$builddir"/.config
	yes "" | make ARCH="$_carch" HOSTCC="$HOSTCC" oldconfig
}

menuconfig() {
	cd "$builddir"
	make ARCH="$_carch" menuconfig
	cp .config "$startdir"/$_config
}

build() {
	unset LDFLAGS
	make ARCH="$_carch" CC="${CC:-gcc}" \
		KBUILD_BUILD_VERSION="$((pkgrel + 1 ))-postmarketOS"

	# Generate master DTB (deviceinfo_bootimg_qcdt)
	dtbTool -s 2048 -p "scripts/dtc/" -o "arch/arm64/boot/dt.img" "arch/arm/boot/"
}

package() {
	# kernel.release
	install -D "$builddir/include/config/kernel.release" \
		"$pkgdir/usr/share/kernel/$_flavor/kernel.release"

	# zImage (find the right one)
	cd "$builddir/arch/$_carch/boot"
	_target="$pkgdir/boot/vmlinuz-$_flavor"
	for _zimg in zImage-dtb Image.gz-dtb *zImage Image; do
		[ -e "$_zimg" ] || continue
		msg "zImage found: $_zimg"
		install -Dm644 "$_zimg" "$_target"
		break
	done
	if ! [ -e "$_target" ]; then
		error "Could not find zImage in $PWD!"
		return 1
	fi

	# Master DTB (deviceinfo_bootimg_qcdt)
	install -Dm644 "$builddir/arch/arm64/boot/dt.img" \
		"$pkgdir/boot/dt.img"
}

sha512sums="2a43545d07b4b477749ac4eaf793e0e7cf105699264d4bd97df20904a3039f421330825dc8c7f9f741387dc3dd9c48b716de6c797048a1f9f358fee97f68fa85  linux-asus-z00t-5fd66aa9219bf9aaa504aa3cb2dae7a3de5238f7.tar.gz
395ec02b12bb376fd558267308b908af9da4111dd18e29639f6c972d8ed2a0cd0a127479adaebe9c618962ea7cddf6d1f63b29b03cd8f5c095c0f9453960f799  config-asus-z00t.aarch64
d80980e9474c82ba0ef1a6903b434d8bd1b092c40367ba543e72d2c119301c8b2d05265740e4104ca1ac5d15f6c4aa49e8776cb44264a9a28dc551e0d1850dcc  compiler-gcc6.h
972e98523d6ef06342e69a09e979bdd86904cf7f9a843b519b37791e531b680182564a2ab537c94629c3589f4e775b2c39de04c64e210a0f8b6f10745c3596f1  01_fix_gcc6_errors.patch
a8c955bf718f155011e980f3d0948be98e1fee5649f418299a4851780543019daf7afa406aa7b0829375645107e4e6fbf241026b0cabe2b2ac895a47df83d2d8  02_mdss_fb_refresh_rate.patch
0e5ebee2f1b0005fcae4f313219c0b6481b3d044c7167e0fb18b72db0eae49aef7b281cd29e0fa1e653fc5585064c990085ca68f920348c3d9d9ea9524d1baa6  05_dtb-fix.patch"
