# Kernel config based on: arch/arm/configs/harpia_defconfig

pkgname="linux-motorola-harpia"
pkgver=3.10.49
pkgrel=2
pkgdesc="Motorola Moto G4 Play kernel fork"
arch="armhf"
_carch="arm"
_flavor="motorola-harpia"
url="https://kernel.org"
license="GPL2"
options="!strip !check !tracedeps"
makedepends="perl sed installkernel bash gmp-dev bc linux-headers elfutils-dev dtbtool xz gcc6"

# Compiler: this kernel was only tested with GCC6. Feel free to make a merge
# request if you find out that it is booting working with newer GCCs as
# well. See <https://postmarketos.org/vendorkernel> for instructions.
if [ "${CC:0:5}" != "gcc6-" ]; then
	CC="gcc6-$CC"
	HOSTCC="gcc6-gcc"
	CROSS_COMPILE="gcc6-$CROSS_COMPILE"
fi

# Source
_repository="android_kernel_motorola_msm8916"
_commit="4c864820053bb70e21cf1e9764baefefd4d2f6b1"
_config="config-${_flavor}.${arch}"
source="
	$pkgname-$_commit.tar.gz::https://github.com/LineageOS/${_repository}/archive/${_commit}.tar.gz
	$_config
	compiler-gcc6.h
"
builddir="$srcdir/${_repository}-${_commit}"

prepare() {
	default_prepare

	# gcc6 support
	cp -v "$srcdir/compiler-gcc6.h" "$builddir/include/linux/"

	# Remove -Werror from all makefiles
	local i
	local makefiles="$(find . -type f -name Makefile)
		$(find . -type f -name Kbuild)"
	for i in $makefiles; do
		sed -i 's/-Werror-/-W/g' "$i"
		sed -i 's/-Werror//g' "$i"
	done

	# Prepare kernel config ('yes ""' for kernels lacking olddefconfig)
	cp "$srcdir"/$_config "$builddir"/.config
	yes "" | make ARCH="$_carch" HOSTCC="$HOSTCC" oldconfig
}

build() {
	unset LDFLAGS
	make ARCH="$_carch" CC="${CC:-gcc}" \
		KBUILD_BUILD_VERSION="$((pkgrel + 1 ))-postmarketOS"

	# Generate master DTB (deviceinfo_bootimg_qcdt)
	dtbTool -s 2048 -p "scripts/dtc/" -o "arch/arm/boot/dt.img" "arch/arm/boot/"
}

package() {
	# kernel.release
	install -D "$builddir/include/config/kernel.release" \
		"$pkgdir/usr/share/kernel/$_flavor/kernel.release"

	# zImage (find the right one)
	cd "$builddir/arch/$_carch/boot"
	_target="$pkgdir/boot/vmlinuz-$_flavor"
	for _zimg in zImage-dtb Image.gz-dtb *zImage Image; do
		[ -e "$_zimg" ] || continue
		msg "zImage found: $_zimg"
		install -Dm644 "$_zimg" "$_target"
		break
	done
	if ! [ -e "$_target" ]; then
		error "Could not find zImage in $PWD!"
		return 1
	fi

	# Master DTB (deviceinfo_bootimg_qcdt)
	install -Dm644 "$builddir/arch/arm/boot/dt.img" \
		"$pkgdir/boot/dt.img"
}

sha512sums="28e70a5af0df65b85c257c4ca455553d38b17dad8d141876854c5a38502114638c8e59440cffcf81c278a6836e39ec0f63ed35dad825c49a8c3f299de7617b80  linux-motorola-harpia-4c864820053bb70e21cf1e9764baefefd4d2f6b1.tar.gz
b6f45b8f832b8be31a0ca8c5c80373532fb7ad08f2343eefb8e9385f863d3e9cc83d74ec03c5b64dbce073a4fb15d6b2df010ea6e1a7d76f35ffe8bfb7f16d8c  config-motorola-harpia.armhf
d80980e9474c82ba0ef1a6903b434d8bd1b092c40367ba543e72d2c119301c8b2d05265740e4104ca1ac5d15f6c4aa49e8776cb44264a9a28dc551e0d1850dcc  compiler-gcc6.h"
