# Kernel config based on: arch/arm64/configs/lineage_ido_defconfig

pkgname="linux-xiaomi-ido"
pkgver=3.10.107
pkgrel=4
pkgdesc="Xiaomi Xiaomi RedMi 3 kernel fork"
arch="aarch64"
_carch="arm64"
_flavor="xiaomi-ido"
url="https://kernel.org"
license="GPL2"
options="!strip !check !tracedeps"
makedepends="perl sed installkernel bash gmp-dev bc linux-headers elfutils-dev dtbtool python gcc6"

# Compiler: this kernel was only tested with GCC6. Feel free to make a merge
# request if you find out that it is booting working with newer GCCs as
# well. See <https://postmarketos.org/vendorkernel> for instructions.
if [ "${CC:0:5}" != "gcc6-" ]; then
	CC="gcc6-$CC"
	HOSTCC="gcc6-gcc"
	CROSS_COMPILE="gcc6-$CROSS_COMPILE"
fi

# Source
_repository="android_kernel_xiaomi_msm8916"
_commit="8f4c7c59fb3a29344af202150030ae712f801d6b"
_config="config-${_flavor}.${arch}"
source="
	$pkgname-$_commit.tar.gz::https://github.com/LineageOS/${_repository}/archive/${_commit}.tar.gz
	$_config
	compiler-gcc6.h
	01_fix_gcc6_errors.patch
"
builddir="$srcdir/${_repository}-${_commit}"

prepare() {
	default_prepare

	# gcc6 support
	cp -v "$srcdir/compiler-gcc6.h" "$builddir/include/linux/"

	# Remove -Werror from all makefiles
	find . -type f -name Makefile -print0 | \
		xargs -0 sed -i 's/-Werror-/-W/g'
	find . -type f -name Makefile -print0 | \
		xargs -0 sed -i 's/-Werror//g'

	# Prepare kernel config ('yes ""' for kernels lacking olddefconfig)
	cp "$srcdir"/$_config "$builddir"/.config
	yes "" | make ARCH="$_carch" HOSTCC="$HOSTCC" oldconfig
}

build() {
	unset LDFLAGS
	make ARCH="$_carch" CC="${CC:-gcc}" \
		KBUILD_BUILD_VERSION="$((pkgrel + 1 ))-postmarketOS"
	dtbTool -s 2048 -p "scripts/dtc/" -o "arch/arm/boot/dt.img" "arch/arm/boot/"
}

package() {
	# kernel.release
	install -D "$builddir/include/config/kernel.release" \
		"$pkgdir/usr/share/kernel/$_flavor/kernel.release"

	# zImage (find the right one)
	cd "$builddir/arch/$_carch/boot"
	_target="$pkgdir/boot/vmlinuz-$_flavor"
	for _zimg in zImage-dtb Image.gz-dtb *zImage Image; do
		[ -e "$_zimg" ] || continue
		msg "zImage found: $_zimg"
		install -Dm644 "$_zimg" "$_target"
		break
	done
	if ! [ -e "$_target" ]; then
		error "Could not find zImage in $PWD!"
		return 1
	fi
	install -Dm644 "$builddir/arch/arm/boot/dt.img" "$pkgdir/boot/dt.img"
}

sha512sums="e22e3cff0819edd2d9f0f16bc952a97773a8b4b36394ab6acf61fd619988d6d0bf1f7d29cba904a09ca0c63209fcedcdf65ee522646193980c5ac6c60e1c3a97  linux-xiaomi-ido-8f4c7c59fb3a29344af202150030ae712f801d6b.tar.gz
c7b9c2900c7d9fa49ea8ceb511092e58aa57e3cf6808e0c9130fac5a5619c7e67b7292e5c4dd23b0a9d3f14f73ba26cbc6c926d5947974395fd602c65324cc1d  config-xiaomi-ido.aarch64
d80980e9474c82ba0ef1a6903b434d8bd1b092c40367ba543e72d2c119301c8b2d05265740e4104ca1ac5d15f6c4aa49e8776cb44264a9a28dc551e0d1850dcc  compiler-gcc6.h
972e98523d6ef06342e69a09e979bdd86904cf7f9a843b519b37791e531b680182564a2ab537c94629c3589f4e775b2c39de04c64e210a0f8b6f10745c3596f1  01_fix_gcc6_errors.patch"
