diff --git a/drivers/video/sprdfb/Kconfig b/drivers/video/sprdfb/Kconfig
index 5c929a5..7f0678c 100755
--- a/drivers/video/sprdfb/Kconfig
+++ b/drivers/video/sprdfb/Kconfig
@@ -305,6 +305,11 @@ config FB_LCD_ST7789V_MCU
 	depends on FB_SC8825 || FB_SCX35 || FB_SCX15
 	default n
 
+config FB_LCD_ST7796S_MIPI
+	boolean "support ST7796S mipi panel"
+	depends on FB_SC8825 || FB_SCX35 || FB_SCX30G
+	default n
+
 config FB_LCD_NT51017_MIPI_LVDS
         boolean "support nt51017 lvds panel"
         depends on FB_SC8825 || FB_SCX35
diff --git a/drivers/video/sprdfb/lcd/Makefile b/drivers/video/sprdfb/lcd/Makefile
index c1b385b..df28587 100755
--- a/drivers/video/sprdfb/lcd/Makefile
+++ b/drivers/video/sprdfb/lcd/Makefile
@@ -27,6 +27,7 @@ obj-$(CONFIG_FB_LCD_S6D77ALA_MIPI_PIKEBJ1MINI) += lcd_s6d77a1a01_mipi_pikebj1min
 obj-$(CONFIG_FB_LCD_SC7798D_MIPI_PIKEBJ1MINI) += lcd_sc7798d_mipi_pikebj1mini.o
 obj-$(CONFIG_FB_LCD_ILI9341) += lcd_ili9341.o
 obj-$(CONFIG_FB_LCD_ST7789V_MCU)  += lcd_st7789v_mcu.o
+obj-$(CONFIG_FB_LCD_ST7796S_MIPI)  += lcd_st7796s_mipi.o
 obj-$(CONFIG_FB_LCD_OTM1283A_MIPI)  += lcd_otm1283a_mipi.o
 obj-$(CONFIG_FB_LCD_NT35502_MIPI) += lcd_nt35502_mipi.o
 obj-$(CONFIG_FB_LCD_VIVA_RGB_SPI) += lcd_hx8363_rgb_spi_viva.o
diff --git a/drivers/video/sprdfb/lcd/lcd_st7796s_mipi.c b/drivers/video/sprdfb/lcd/lcd_st7796s_mipi.c
new file mode 100644
index 0000000..2096e01
--- /dev/null
+++ b/drivers/video/sprdfb/lcd/lcd_st7796s_mipi.c
@@ -0,0 +1,252 @@
+/* drivers/video/sprdfb/lcd/lcd_st7796s_mipi.c
+ *
+ * Support for ST7796S mipi LCD device
+ *
+ * Copyright (C) 2010 Spreadtrum
+ *
+ * This software is licensed under the terms of the GNU General Public
+ * License version 2, as published by the Free Software Foundation, and
+ * may be copied, distributed, and modified under those terms.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ */
+
+#include <linux/kernel.h>
+#include <linux/bug.h>
+#include <linux/delay.h>
+#include "../sprdfb_panel.h"
+
+#define MAX_DATA   100
+
+typedef struct LCM_Init_Code_tag {
+	unsigned int tag;
+	unsigned char data[MAX_DATA];
+}LCM_Init_Code;
+
+typedef struct LCM_force_cmd_code_tag{
+	unsigned int datatype;
+	LCM_Init_Code real_cmd_code;
+}LCM_Force_Cmd_Code;
+
+#define LCM_TAG_SHIFT 24
+#define LCM_TAG_MASK  ((1 << 24) -1)
+#define LCM_SEND(len) ((1 << LCM_TAG_SHIFT)| len)
+#define LCM_SLEEP(ms) ((2 << LCM_TAG_SHIFT)| ms)
+
+#define LCM_TAG_SEND  (1<< 0)
+#define LCM_TAG_SLEEP (1 << 1)
+
+static LCM_Init_Code init_data[] = {
+	/*{0xF0, 1, {0xC3}}, COMMAND SET CONTROL: ENABLE COMMAND 2 part I
+	{0xF0, 1, {0x96}}, COMMAND SET CONTROL: ENABLE COMMAND 2 part II
+	{0x36, 1, {0x86}}, MADCTL (memory data access control): mirror framebuffer, 
+	{0xB4, 1, {0x01}}, DIC (display inversion control) : 1-dot inversion
+	{0x3A, 1, {0x55}}, Interface pixel format: 18-bit//0x55
+	{0xB7, 1, {0x06}}, Entry Mode Set: normal display
+	{0xB9, 2, {0x02,0XC0}},
+	{0x35, 1, {0x00}}, Tearing effect line: disabled
+	{0x44, 2, {0x00,0x00}}, Set tear scanline: 0
+	
+	{0xE8, 8, {0x40,0x8a,0x00,0x00,0x29,0x19,0xa5,0x33}}, Display output ctrl adjust
+	{0xC5, 1, {0x25}}, VCOM control: 1.225
+	{0xC2, 1, {0xA5}}, PWR3 Power control: low
+	GAMMA CONTROL
+	{0xE0, 14, {0xF0,0x00,0x03,0x0b,0x0c,0x29,0x2e,0x44,0x41,0x17,0x11,0x13,0x16,0x1b}},
+	{0xE1, 14, {0xF0,0x00,0x02,0x06,0x06,0x24,0x2a,0x43,0x3e,0x2d,0x1a,0x16,0x13,0x17}},
+	{0xEC, 3,  {0x00,0x00,0x01}}, 
+	
+	{0xF0, 1, {0x3C}}, COMMAND SET CONTROL
+	{0xF0, 1, {0x69}}, COMMAND SET CONTROL
+
+	{0x29, 1, {0x00}},
+	{REGFLAG_DELAY, 20, {}},*/
+	{LCM_SEND(1), {0xC3}},
+	{LCM_SEND(1), {0x96}},
+	{LCM_SEND(1), {0x86}}, 
+	{LCM_SEND(1), {0x01}},
+	{LCM_SEND(1), {0x55}},//0x55
+	{LCM_SEND(1), {0x06}},
+	{LCM_SEND(2), {0x02,0XC0}},
+	{LCM_SEND(1), {0x00}},
+	{LCM_SEND(2), {0x00,0x00}},
+	
+	{LCM_SEND(8), {0x40,0x8a,0x00,0x00,0x29,0x19,0xa5,0x33}},
+	{LCM_SEND(1), {0x25}},
+	{LCM_SEND(1), {0xA5}},  
+	
+	{LCM_SEND(14), {0xF0,0x00,0x03,0x0b,0x0c,0x29,0x2e,0x44,0x41,0x17,0x11,0x13,0x16,0x1b}},
+	{LCM_SEND(14), {0xF0,0x00,0x02,0x06,0x06,0x24,0x2a,0x43,0x3e,0x2d,0x1a,0x16,0x13,0x17}},
+	{LCM_SEND(3),  {0x00,0x00,0x01}},
+	
+	{LCM_SEND(1), {0x3C}},
+	{LCM_SEND(1), {0x69}},
+
+	{LCM_SEND(1), 1, {0x00}},
+	{LCM_SLEEP(20)},
+};
+
+static LCM_Init_Code sleep_in[] =  {
+	{LCM_SEND(1), {0x28}},
+	{LCM_SLEEP(50)}, 	//>150ms
+	{LCM_SEND(1), {0x10}},
+	{LCM_SLEEP(120)},	//>150ms
+};
+
+static LCM_Init_Code sleep_out[] =  {
+	{LCM_SEND(1), {0x11}},
+	{LCM_SLEEP(120)},//>120ms
+	{LCM_SEND(1), {0x29}},
+	{LCM_SLEEP(50)}, //>20ms
+};
+
+static int32_t st7796s_mipi_init(struct panel_spec *self)
+{
+	int32_t i;
+	LCM_Init_Code *init = init_data;
+	unsigned int tag;
+
+	mipi_set_cmd_mode_t mipi_set_cmd_mode = self->info.mipi->ops->mipi_set_cmd_mode;
+	mipi_dcs_write_t mipi_dcs_write = self->info.mipi->ops->mipi_dcs_write;
+	mipi_eotp_set_t mipi_eotp_set = self->info.mipi->ops->mipi_eotp_set;
+
+	printk("kernel ili9486s1_mipi_init\n");
+
+	mipi_set_cmd_mode();
+	mipi_eotp_set(0,0);
+
+	for(i = 0; i < ARRAY_SIZE(init_data); i++){
+		tag = (init->tag >>24);
+		if(tag & LCM_TAG_SEND){
+			mipi_dcs_write(init->data, (init->tag & LCM_TAG_MASK));
+			udelay(20);
+		}else if(tag & LCM_TAG_SLEEP){
+			msleep(init->tag & LCM_TAG_MASK);
+		}
+		init++;
+	}
+	mipi_eotp_set(0,0);
+
+	return 0;
+}
+
+
+static uint32_t st7796s_readid(struct panel_spec *self)
+{
+	printk("lcd_dummy read id!\n");
+	printk("lcd_dummy read id success!\n");
+	return 0x7796;
+}
+
+
+static int32_t st7796s_enter_sleep(struct panel_spec *self, uint8_t is_sleep)
+{
+	int32_t i;
+	LCM_Init_Code *sleep_in_out = NULL;
+	unsigned int tag;
+	int32_t size = 0;
+
+	mipi_set_cmd_mode_t mipi_set_cmd_mode = self->info.mipi->ops->mipi_set_cmd_mode;
+	mipi_dcs_write_t mipi_dcs_write = self->info.mipi->ops->mipi_dcs_write;
+	mipi_eotp_set_t mipi_eotp_set = self->info.mipi->ops->mipi_eotp_set;
+
+	printk("kernel nt35502_enter_sleep, is_sleep = %d\n", is_sleep);
+
+	if(is_sleep){
+		sleep_in_out = sleep_in;
+		size = ARRAY_SIZE(sleep_in);
+	}else{
+		sleep_in_out = sleep_out;
+		size = ARRAY_SIZE(sleep_out);
+	}
+
+	mipi_set_cmd_mode();
+	mipi_eotp_set(0,0);
+
+	for(i = 0; i <size ; i++){
+		tag = (sleep_in_out->tag >>24);
+		if(tag & LCM_TAG_SEND){
+			mipi_dcs_write(sleep_in_out->data, (sleep_in_out->tag & LCM_TAG_MASK));
+		}else if(tag & LCM_TAG_SLEEP){
+			msleep(sleep_in_out->tag & LCM_TAG_MASK);
+		}
+		sleep_in_out++;
+	}
+	mipi_eotp_set(0,0);
+
+	return 0;
+}
+
+/* esd check disabled
+static int32_t st7796s_check_esd(struct panel_spec *self)
+{
+	pr_debug("dummy_check_esd!\n");
+	pr_debug("dummy_check_esd OK!\n");
+	return 1;	
+} */
+
+
+static struct panel_operations lcd_st7796s_mipi_operations = {
+	.panel_init = st7796s_mipi_init,
+	.panel_readid = st7796s_readid,
+	.panel_enter_sleep = st7796s_enter_sleep,
+	//.panel_esd_check = dummy_check_esd,
+};
+
+
+static struct timing_rgb lcd_st7796s_mipi_timing = {
+	/* unit: pixel */
+	.hfp = 65,  //Horizontal front porch
+	.hbp = 10,  //Horizontal back porch
+	.hsync = 10,//6,
+	/*unit: line*/
+	.vfp = 8, //Vertical front porch
+	.vbp = 10, //Vertical back porch
+	.vsync = 3,
+};
+
+static struct info_mipi lcd_st7796s_mipi_info = {
+	.work_mode  = SPRDFB_MIPI_MODE_VIDEO,
+	.video_bus_width = 18, /*18,16*/
+	.lan_number = 1,
+	.phy_feq = 340*1000,
+	.h_sync_pol = SPRDFB_POLARITY_NEG,
+	.v_sync_pol = SPRDFB_POLARITY_NEG,
+	.de_pol = SPRDFB_POLARITY_POS,
+	.te_pol = SPRDFB_POLARITY_POS,
+	.color_mode_pol = SPRDFB_POLARITY_POS,
+	.shut_down_pol = SPRDFB_POLARITY_NEG,
+	.timing = &lcd_st7796s_mipi_timing,
+	.ops = NULL,
+};
+
+// DONE 
+
+struct panel_spec lcd_st7796s_mipi_spec = {
+	.width = 320,
+	.height = 480,
+	.fps = 60,
+	.type = LCD_MODE_DSI,
+	.direction = LCD_DIRECT_NORMAL,
+	//.is_clean_lcd = true,
+	.info = {
+		.mipi = &lcd_st7796s_mipi_info
+	},
+	.ops = &lcd_st7796s_mipi_operations,
+};
+
+struct panel_cfg lcd_st7796s_mipi = {
+	.dev_id = SPRDFB_MAINLCD_ID,
+	.lcd_id = 0x7796,
+	.lcd_name = "lcd_st7796s_mipi",
+	.panel = &lcd_st7796s_mipi_spec,
+};
+
+static int __init lcd_st7796s_mipi_init(void)
+{
+	return sprdfb_panel_register(&lcd_st7796s_mipi);
+}
+
+subsys_initcall(lcd_st7796s_mipi_init);
