# Kernel config based on: arch/arm/configs/msm8610-zte_defconfig

pkgname="linux-zte-kis3"
pkgver=3.4.0
pkgrel=2
pkgdesc="ZTE Kis 3 kernel fork"
arch="armhf"
_carch="arm"
_flavor="zte-kis3"
url="https://kernel.org"
license="GPL2"
options="!strip !check !tracedeps"
makedepends="perl sed installkernel bash gmp-dev bc linux-headers elfutils-dev dtbtool xz gcc6"

# Compiler: this kernel was only tested with GCC6. Feel free to make a merge
# request if you find out that it is booting working with newer GCCs as
# well. See <https://postmarketos.org/vendorkernel> for instructions.
if [ "${CC:0:5}" != "gcc6-" ]; then
	CC="gcc6-$CC"
	HOSTCC="gcc6-gcc"
	CROSS_COMPILE="gcc6-$CROSS_COMPILE"
fi

# Source
_repository="android_kernel_zte_msm8610"
_commit="b55a46067bb75d8a290b2cc0e07f5fb3d8207cb1"
_config="config-${_flavor}.${arch}"
source="
	$pkgname-$_commit.tar.gz::https://github.com/KonstaT/${_repository}/archive/${_commit}.tar.gz
	$_config
	compiler-gcc6.h
	00_fix_return_address.patch
	02_gpu-msm-fix-gcc5-compile.patch
"
builddir="$srcdir/${_repository}-${_commit}"

prepare() {
	default_prepare

	# gcc6 support
	cp -v "$srcdir/compiler-gcc6.h" "$builddir/include/linux/"

	# Remove -Werror from all makefiles
	local i
	local makefiles="$(find . -type f -name Makefile)
		$(find . -type f -name Kbuild)"
	for i in $makefiles; do
		sed -i 's/-Werror-/-W/g' "$i"
		sed -i 's/-Werror//g' "$i"
	done

	# Prepare kernel config ('yes ""' for kernels lacking olddefconfig)
	cp "$srcdir"/$_config "$builddir"/.config
	yes "" | make ARCH="$_carch" HOSTCC="$HOSTCC" oldconfig
}

build() {
	unset LDFLAGS
	make ARCH="$_carch" CC="${CC:-gcc}" \
		KBUILD_BUILD_VERSION="$((pkgrel + 1 ))-postmarketOS"

	# Generate master DTB (deviceinfo_bootimg_qcdt)
	dtbTool -s 2048 -p "scripts/dtc/" -o "arch/arm/boot/dt.img" "arch/arm/boot/"
}

package() {
	# kernel.release
	install -D "$builddir/include/config/kernel.release" \
		"$pkgdir/usr/share/kernel/$_flavor/kernel.release"

	# zImage (find the right one)
	cd "$builddir/arch/$_carch/boot"
	_target="$pkgdir/boot/vmlinuz-$_flavor"
	for _zimg in zImage-dtb Image.gz-dtb *zImage Image; do
		[ -e "$_zimg" ] || continue
		msg "zImage found: $_zimg"
		install -Dm644 "$_zimg" "$_target"
		break
	done
	if ! [ -e "$_target" ]; then
		error "Could not find zImage in $PWD!"
		return 1
	fi

	# Master DTB (deviceinfo_bootimg_qcdt)
	install -Dm644 "$builddir/arch/arm/boot/dt.img" \
		"$pkgdir/boot/dt.img"
}

sha512sums="5759d54232e0c83e71896fc4c859fe8554731678defa337ec9da441505e03fb2f3b795fb68b35dec8e0fc6a920e82f03cd986badc05cf55c993d22085620bebc  linux-zte-kis3-b55a46067bb75d8a290b2cc0e07f5fb3d8207cb1.tar.gz
1f9c7131401569c5a784b7a63744800a58dd226d5beabba93ae2a64b98b71233f4bcbe15ea5ce8170a85afc9f1271c82e7b92136d5c7023d87064f403d1a02d7  config-zte-kis3.armhf
d80980e9474c82ba0ef1a6903b434d8bd1b092c40367ba543e72d2c119301c8b2d05265740e4104ca1ac5d15f6c4aa49e8776cb44264a9a28dc551e0d1850dcc  compiler-gcc6.h
ea1d3b5a234fa565e3c1a792de48f4fc4e6023d281d303c8e319c7ef28edc5739ab0e4dea0139a41f0a5c7d03e27921ccaa214fd0ac5c72245a094ce60128864  00_fix_return_address.patch
7be03a9e78b7ac330a54b1f00509caa0621a95c0c55901878ad757f9dd69cc05ba2c8b5ea987063ae1224f92c4d090d515fa5d369e7755181a4871b0d0f82881  02_gpu-msm-fix-gcc5-compile.patch"
