diff --git a/drivers/input/touchscreen/synaptics_driver_s3320.c b/drivers/input/touchscreen/synaptics_driver_s3320.c
index 79b184a..f3d3872 100644
--- a/drivers/input/touchscreen/synaptics_driver_s3320.c
+++ b/drivers/input/touchscreen/synaptics_driver_s3320.c
@@ -2105,7 +2105,6 @@ static int	synaptics_input_init(struct synaptics_ts_data *ts)
 	set_bit(EV_ABS, ts->input_dev->evbit);
 	set_bit(EV_KEY, ts->input_dev->evbit);
 	set_bit(ABS_MT_TOUCH_MAJOR, ts->input_dev->absbit);
-	set_bit(ABS_MT_WIDTH_MAJOR,ts->input_dev->absbit);
 	set_bit(ABS_MT_POSITION_X, ts->input_dev->absbit);
 	set_bit(ABS_MT_POSITION_Y, ts->input_dev->absbit);
 	set_bit(INPUT_PROP_DIRECT, ts->input_dev->propbit);
