SectionVerb {
        EnableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='PRI_MI2S_RX Audio Mixer MultiMedia1' 1"
                cset "name='MultiMedia1 Mixer TERT_MI2S_TX' 1"
        ]

        DisableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='PRI_MI2S_RX Audio Mixer MultiMedia1' 0"
                cset "name='MultiMedia1 Mixer TERT_MI2S_TX' 0"
        ]

        Value {
                TQ "HiFi"
                PlaybackPCM "hw:msm8920sku7sndc,0"
                CapturePCM "hw:msm8920sku7sndc,0"
        }

}

SectionDevice."Speaker" {
        Comment "Speaker"

        ConflictingDevice [
        ]

        EnableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='MI2S_RX Channels' One"
                cset "name='RX2 MIX1 INP1' RX2"
                cset "name='RDAC2 MUX' RX2"
                cset "name='HPHR' Switch"
                cset "name='Lineout_1 amp' ENABLE"
                cset "name='PRI_MI2S_RX Audio Mixer MultiMedia1' 1"
        ]

        DisableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='MI2S_RX Channels' One"
                cset "name='RX2 MIX1 INP1' ZERO"
                cset "name='RDAC2 MUX' ZERO"
                cset "name='HPHR' ZERO"
                cset "name='Lineout_1 amp' DISABLE"
                cset "name='PRI_MI2S_RX Audio Mixer MultiMedia1' 0"
        ]

        Value {
                PlaybackChannels "2"
        }

}

SectionDevice."Headphones" {
        Comment "Headset"

        ConflictingDevice [
        ]

        EnableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='MI2S_RX Channels' Two"
                cset "name='RX1 MIX1 INP1' RX1"
                cset "name='RX2 MIX1 INP1' RX2"
                cset "name='RDAC2 MUX' RX2"
                cset "name='HPHL' Switch"
                cset "name='HPHR' Switch"
                cset "name='headset amp' ENABLE"
                cset "name='PRI_MI2S_RX Audio Mixer MultiMedia1' 1"
        ]

        DisableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='MI2S_RX Channels' One"
                cset "name='RX1 MIX1 INP1' ZERO"
                cset "name='RX2 MIX1 INP1' ZERO"
                cset "name='RDAC2 MUX' ZERO"
                cset "name='HPHL' ZERO"
                cset "name='HPHR' ZERO"
                cset "name='headset amp' DISABLE"
                cset "name='PRI_MI2S_RX Audio Mixer MultiMedia1' 0"
        ]

        Value {
                PlaybackChannels "2"
        }

}

SectionDevice."Handset" {
        Comment "Handset earpiece"

        ConflictingDevice [
                "Speaker"
                "SpeakerMic"
                "Headphones"
        ]

        EnableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='RX1 MIX1 INP1' RX1"
                cset "name='RDAC2 MUX' RX1"
                cset "name='RX1 Digital Volume' 86"
                cset "name='EAR PA Gain' POS_6_DB"
                cset "name='EAR_S' Switch"
                cset "name='PRI_MI2S_RX Audio Mixer MultiMedia1' 1"
        ]

        DisableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='RX1 MIX1 INP1' ZERO"
                cset "name='RDAC2 MUX' ZERO"
                cset "name='RX1 Digital Volume' 86"
                cset "name='EAR PA Gain' POS_6_DB"
                cset "name='EAR_S' ZERO"
                cset "name='PRI_MI2S_RX Audio Mixer MultiMedia1' 0"
        ]

        Value {
                PlaybackChannels "2"
        }

}

SectionDevice."HandsetMic" {
        Comment "Handset microphone"

        ConflictingDevice [
                "Speaker"
                "SpeakerMic"
                "HeadsetMic"
        ]

        EnableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='ADC1 Volume' 6"
                cset "name='DEC1 MUX' ADC1"
                cset "name='IIR1 INP1 MUX' DEC1"
                cset "name='MultiMedia1 Mixer TERT_MI2S_TX' 1"
        ]

        DisableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='ADC1 Volume' 4"
                cset "name='DEC1 MUX' ZERO"
                cset "name='MultiMedia1 Mixer TERT_MI2S_TX' 0"
        ]

        Value {
                CaptureChannels "2"
        }

}

SectionDevice."SpeakerMic" {
        Comment "Handset microphone for speaker-mode"

        ConflictingDevice [
                "Handset"
                "HandsetMic"
                "HeadsetMic"
        ]

        EnableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='ADC1 Volume' 6"
                cset "name='DEC1 MUX' ADC1"
                cset "name='IIR1 INP1 MUX' DEC1"
                cset "name='MultiMedia1 Mixer TERT_MI2S_TX' 1"
        ]

        DisableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='ADC1 Volume' 4"
                cset "name='DEC1 MUX' ZERO"
                cset "name='MultiMedia1 Mixer TERT_MI2S_TX' 0"
        ]

        Value {
                CaptureChannels "2"
        }

}

SectionDevice."HeadsetMic" {
        Comment "Headset microphone"

        ConflictingDevice [
                "HandsetMic"
                "SpeakerMic"
        ]

        EnableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='ADC2 Volume' 6"
                cset "name='DEC1 MUX' ADC2"
                cset "name='ADC2 MUX' INP2"
                cset "name='IIR1 INP1 MUX' DEC1"
                cset "name='MultiMedia1 Mixer TERT_MI2S_TX' 1"
        ]

        DisableSequence [
                cdev "hw:msm8920sku7sndc"

                cset "name='ADC2 Volume' 4"
                cset "name='DEC1 MUX' ZERO"
                cset "name='ADC2 MUX' ZERO"
                cset "name='MultiMedia1 Mixer TERT_MI2S_TX' 0"
        ]

        Value {
                CaptureChannels "2"
        }

}

