# udev rules file
# All device names can be read from weston's logfile

# Touchscreen (use 'weston-calibrator' to calibrate)
SUBSYSTEM=="input", ATTRS{name}=="synaptics_dsx_i2c", \
ENV{ID_INPUT}="1", ENV{ID_INPUT_TOUCHSCREEN}="1" \
ENV{WL_CALIBRATION}="1.013786 0.035310 -24.920929 -0.008370 0.990421 12.094299"

