From 08eb3117ef1d2eb9f634920bc671125284d80e7b Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Fri, 4 Jun 2021 00:00:04 +0200
Subject: ARM: dts: ux500: Skomer regulator fixes

AUX2 has slightly wrong voltage and AUX5 doesn't need to be
always on.

Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
---
 arch/arm/boot/dts/ste-ux500-samsung-skomer.dts | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

diff --git a/arch/arm/boot/dts/ste-ux500-samsung-skomer.dts b/arch/arm/boot/dts/ste-ux500-samsung-skomer.dts
index feee836c6c56c..368abbd9b10b7 100644
--- a/arch/arm/boot/dts/ste-ux500-samsung-skomer.dts
+++ b/arch/arm/boot/dts/ste-ux500-samsung-skomer.dts
@@ -307,10 +307,10 @@
 					};
 
 					ab8500_ldo_aux2 {
-						/* Supplies the Cypress TMA140 touchscreen only with 3.3V */
+						/* Supplies the Cypress TMA140 touchscreen only with 3.0V */
 						regulator-name = "AUX2";
-						regulator-min-microvolt = <3300000>;
-						regulator-max-microvolt = <3300000>;
+						regulator-min-microvolt = <3000000>;
+						regulator-max-microvolt = <3000000>;
 					};
 
 					ab8500_ldo_aux3 {
@@ -329,9 +329,9 @@
 
 					ab8500_ldo_aux5 {
 						regulator-name = "AUX5";
+						/* Intended for 1V8 for touchscreen but actually left unused */
 						regulator-min-microvolt = <1050000>;
 						regulator-max-microvolt = <2790000>;
-						regulator-always-on;
 					};
 
 					ab8500_ldo_aux6 {
-- 
cgit 1.2.3-1.el7
