(footprint "L_FXL0420" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61807CCD)
  (fp_text reference "REF**" (at 0 -4.6 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ed682139-1330-4e98-99ae-b9ba2f33be87)
  )
  (fp_text value "L_FXL0420" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1549ab4d-45ca-47ac-9e20-53d95da7d830)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a79ecd24-f751-4d6c-a73b-984f9ff384f6)
  )
  (fp_line (start -2.3 -1.4) (end -2.3 -2.3) (layer "F.SilkS") (width 0.12) (tstamp 1e82d8de-1660-44f7-831a-e6f96eb128a3))
  (fp_line (start -2.3 -2.3) (end 2.3 -2.3) (layer "F.SilkS") (width 0.12) (tstamp 3cd85e78-9703-431c-b5f2-c33808b9674a))
  (fp_line (start -2.3 1.4) (end -2.3 2.3) (layer "F.SilkS") (width 0.12) (tstamp 7e3e0cc6-3be2-4838-a837-f8cd0d2f9ca1))
  (fp_line (start -2.3 2.3) (end 2.3 2.3) (layer "F.SilkS") (width 0.12) (tstamp 7fe66566-eac4-4bde-896a-848bb6c8b4a2))
  (fp_line (start 2.3 -2.3) (end 2.3 -1.4) (layer "F.SilkS") (width 0.12) (tstamp cbc32d52-2207-445b-959e-cf47f2b132fd))
  (fp_line (start 2.3 2.3) (end 2.3 1.4) (layer "F.SilkS") (width 0.12) (tstamp fb9aaf8c-f040-4bfd-a30d-d67de5def305))
  (fp_rect (start -2.7 -2.5) (end 2.7 2.5) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 3864d017-ff37-4727-8da0-9025486eac11))
  (fp_rect (start -2.1 -2.1) (end 2.1 2.1) (layer "F.Fab") (width 0.1) (fill none) (tstamp 78b09a9b-8c2d-486f-a825-bcc1e45e06dd))
  (pad "1" smd rect (at -1.85 0) (size 1.5 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 840f58fc-632f-4855-a4fe-63f2ca751ee3))
  (pad "2" smd rect (at 1.85 0) (size 1.5 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp d4428660-2e7a-425f-af90-b0e7fa1cf6e6))
)
