(footprint "L_MAPM1040F" (version 20210824) (generator pcbnew) (layer "F.Cu")
  (tedit 61807CD3)
  (fp_text reference "REF**" (at 0 -6.7 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ed682139-1330-4e98-99ae-b9ba2f33be87)
  )
  (fp_text value "L_MAPM1040F" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1549ab4d-45ca-47ac-9e20-53d95da7d830)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a79ecd24-f751-4d6c-a73b-984f9ff384f6)
  )
  (fp_line (start -5.7 -2.2) (end -5.7 -5.7) (layer "F.SilkS") (width 0.12) (tstamp 0daba2ef-9fb3-4a31-91da-eeaded0eab2b))
  (fp_line (start 5.7 -5.7) (end 5.7 -2.2) (layer "F.SilkS") (width 0.12) (tstamp 7192a7b6-9708-402e-97e6-d96d458bb3d2))
  (fp_line (start -5.7 5.7) (end -5.7 2.2) (layer "F.SilkS") (width 0.12) (tstamp 86937ab2-f407-4f45-9bc1-15a0b67b7ba8))
  (fp_line (start 5.7 2.2) (end 5.7 5.7) (layer "F.SilkS") (width 0.12) (tstamp 9ec82587-f52f-4809-87ca-0ab42d0358d9))
  (fp_line (start 5.7 5.7) (end -5.7 5.7) (layer "F.SilkS") (width 0.12) (tstamp a0aa5c23-4c81-4419-be32-219f4ad31065))
  (fp_line (start -5.7 -5.7) (end 5.7 -5.7) (layer "F.SilkS") (width 0.12) (tstamp b4e95e5c-19a5-4feb-8fe7-7d5242d758bf))
  (fp_rect (start -7 -5.9) (end 7 5.9) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 64a6b206-2761-4977-8b5f-b0696d7073c7))
  (fp_rect (start -5.5 -5.5) (end 5.5 5.5) (layer "F.Fab") (width 0.1) (fill none) (tstamp 78b09a9b-8c2d-486f-a825-bcc1e45e06dd))
  (pad "1" smd rect (at -4.9 0) (size 3.8 4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 840f58fc-632f-4855-a4fe-63f2ca751ee3))
  (pad "2" smd rect (at 4.9 0) (size 3.8 4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp d4428660-2e7a-425f-af90-b0e7fa1cf6e6))
)
