39436226710237
footprints
472720024
47272-0024
Connector
0
24
21
footprints
AXE520124


0
24
21
footprints
AXE550127


0
54
51
footprints
AXT524124


0
28
25
footprints
BGA-96_9.0x14.0mm_P0.8mm
BGA-96, http://www.mouser.com/ds/2/198/43-46TR16640B-81280BL-706483.pdf
BGA-96
0
96
96
footprints
HRS_FH26W-39S-0.3SHW(60)


0
41
41
footprints
Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal_Reversed
Hirose FH12, FFC/FPC connector, FH12-40S-0.5SH, 40 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator
connector Hirose FH12 horizontal
0
42
41
footprints
L_1212
Inductor, 3.0mmx3.0mm
inductor vishay ihlp smd
0
2
2
footprints
L_CommonModeChoke_Panasonic_EXC14CE
Coilcraft 0603USB Series Common Mode Choke, https://www.coilcraft.com/pdfs/0603usb.pdf
surface mount common mode bead
0
4
4
footprints
L_FXL0420


0
2
2
footprints
L_MAPM0630F


0
2
2
footprints
L_MAPM1040F


0
2
2
footprints
MPS_QFN-16_3x3mm_P0.4mm
QFN, 16 Pin (https://www.onsemi.com/pub/Collateral/NCN4555-D.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py
QFN NoLead
0
16
16
footprints
MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm_ThermalVias_0.3
MSOP, 10 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3805fg.pdf#page=18), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
20
11
footprints
Molex_200528-0060_1x06-1MP_P1.00mm_Horizontal_Reversed
Molex Molex 1.00mm Pitch Easy-On BackFlip, Right-Angle, Bottom Contact FFC/FPC, 200528-0060, 6 Circuits (https://www.molex.com/pdm_docs/sd/2005280060_sd.pdf), generated with kicad-footprint-generator
connector Molex  top entry
0
8
7
footprints
QFN-28-1EP_4x5mm_P0.5mm_EP2.65x3.65mm_ThermalVias_0.3
QFN, 28 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/3555fe.pdf#page=32), generated with kicad-footprint-generator ipc_noLead_generator.py
QFN NoLead
0
48
29
footprints
QFN-48-1EP_7x7mm_P0.5mm_EP4.1x4.1mm_ThermalVias
QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py
QFN NoLead
0
71
49
footprints
RP2040-QFN-56
QFN, 56 Pin (http://www.cypress.com/file/416486/download#page=40), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py
QFN DFN_QFN
0
70
57
footprints
TE_5-2069716-3_1x40-1MP_P0.5mm_Horizontal
TE FPC connector, 40 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0
te fpc 1734839
0
44
41
footprints
TE_1612503-1


0
7
6
footprints
TE_1735413-1
SATA, Receptacle, Cable-to-Board, 13 Position, 6P + 7P, Slimline Connector Profile, Right Angle, Surface Mount

0
15
14
footprints
TE_2023246-2
SATA, Receptacle, Cable-to-Board, 22 Position, 7P + 15P, Standard Connector Profile, Right Angle, Surface Mount

0
24
23
footprints
USB-306A-B-SU
USB TYPE C, RA RCPT PCB, Hybrid, https://www.amphenolcanada.com/StockAvailabilityPrice.aspx?From=&PartNum=12401548E4%7e2A
USB C Type-C Receptacle Hybrid
0
28
25
footprints
Xilinx_FTG256
Artix-7 BGA, 16x16 grid, 17x17mm package, 1mm pitch; https://www.xilinx.com/support/documentation/user_guides/ug475_7Series_Pkg_Pinout.pdf#page=269, NSMD pad definition Appendix A
BGA 256 1 FT256 FTG256
0
256
256
