# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="PINE64 PinePhone Don't be evil devkit"
deviceinfo_manufacturer="PINE64"
deviceinfo_codename="pine64-dontbeevil"
deviceinfo_year="2019"
deviceinfo_dtb_shortts="allwinner/sun50i-a64-dontbeevil"
deviceinfo_dtb_longts="allwinner/sun50i-a64-dontbeevil-longts"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_chassis="handset"
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
deviceinfo_screen_width="720"
deviceinfo_screen_height="1440"

# Bootloader related
deviceinfo_flash_method="none"
deviceinfo_generate_legacy_uboot_initfs="true"
deviceinfo_sd_embed_firmware="u-boot/pine64-lts/u-boot-sunxi-with-spl.bin:8"
