# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="PocketBook 614 Plus"
deviceinfo_manufacturer="PocketBook"
deviceinfo_codename="pocketbook-614-plus"
deviceinfo_year="2017"
deviceinfo_arch="armv7"

# Device related
deviceinfo_chassis="tablet"
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
# There is no driver for electronic paper used in this device yet.
deviceinfo_no_framebuffer="true"
deviceinfo_getty="ttyS0;115200"

# Bootloader related
deviceinfo_flash_method="none"
deviceinfo_append_dtb="false"
deviceinfo_dtb="sun5i-a13-pocketbook-614-plus"
deviceinfo_kernel_cmdline="console=ttyS0,115200 earlycon"
deviceinfo_generate_extlinux_config="true"
deviceinfo_sd_embed_firmware="u-boot/pocketbook-614-plus/u-boot-sunxi-with-spl.bin:8"
deviceinfo_boot_part_start="8192"
