# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Fairphone 3"
deviceinfo_manufacturer="Fairphone"
deviceinfo_codename="fairphone-fp3"
deviceinfo_year="2019"
deviceinfo_dtb_mainline="qcom/sdm632-fairphone-fp3"
deviceinfo_append_dtb_mainline="true"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_chassis="handset"
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1080"
deviceinfo_screen_height="2160"
deviceinfo_getty="ttyMSM0;115200"
deviceinfo_gpu_accelerated="true"

# Bootloader related
deviceinfo_flash_method="fastboot"
deviceinfo_kernel_cmdline_downstream="console=ttyMSM0,115200,n8 androidboot.console=ttyMSM0 androidboot.hardware=qcom msm_rtb.filter=0x237 ehci-hcd.park=3 lpm_levels.sleep_disabled=1 androidboot.bootdevice=7824900.sdhci earlycon=msm_serial_dm,0x78af000 androidboot.usbconfigfs=true loop.max_part=7 buildvariant=user"
deviceinfo_kernel_cmdline_mainline="console=ttyMSM0,115200"
deviceinfo_generate_bootimg="true"
deviceinfo_generate_extlinux_config="true"
deviceinfo_bootimg_qcdt="false"
deviceinfo_bootimg_mtk_mkimage="false"
deviceinfo_bootimg_dtb_second="false"
deviceinfo_flash_fastboot_partition_vbmeta="vbmeta"
deviceinfo_flash_offset_base="0x80000000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x01000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x00000100"
deviceinfo_flash_pagesize="2048"
