From 788a8f664a92e775fa61f03dfe312e4a482c5242 Mon Sep 17 00:00:00 2001
From: JuniorJPDJ <git@juniorjpdj.pl>
Date: Sun, 28 Mar 2021 03:07:12 +0200
Subject: [PATCH] configs: add lark-freeme-70-2s

---
 configs/lark-freeme-70-2s_defconfig | 26 ++++++++++++++++++++++++++
 1 file changed, 26 insertions(+)
 create mode 100644 configs/lark-freeme-70-2s_defconfig

diff --git a/configs/lark-freeme-70-2s_defconfig b/configs/lark-freeme-70-2s_defconfig
new file mode 100644
index 0000000000..c6687f632a
--- /dev/null
+++ b/configs/lark-freeme-70-2s_defconfig
@@ -0,0 +1,26 @@
+CONFIG_ARM=y
+CONFIG_ARCH_SUNXI=y
+CONFIG_SPL=y
+CONFIG_MACH_SUN4I=y
+CONFIG_DRAM_CLK=360
+CONFIG_DRAM_EMR1=4
+CONFIG_MMC0_CD_PIN="PH1"
+CONFIG_USB0_VBUS_DET="PH5"
+CONFIG_USB0_VBUS_PIN="PB9"
+CONFIG_USB0_ID_DET="PH4"
+# CONFIG_VIDEO_HDMI is not set
+CONFIG_VIDEO_LCD_MODE="x:800,y:480,depth:18,pclk_khz:33000,le:87,ri:40,up:31,lo:13,hs:1,vs:1,sync:3,vmode:0"
+CONFIG_VIDEO_LCD_POWER="PH8"
+CONFIG_VIDEO_LCD_BL_EN="PH7"
+CONFIG_VIDEO_LCD_BL_PWM="PB2"
+CONFIG_NR_DRAM_BANKS=1
+CONFIG_SPL_TEXT_BASE=0x60
+# CONFIG_SYS_MALLOC_CLEAR_ON_INIT is not set
+CONFIG_SPL_I2C_SUPPORT=y
+CONFIG_DEFAULT_DEVICE_TREE="sun4i-a10-lark-freeme-70-2s"
+CONFIG_USB_MUSB_HOST=y
+CONFIG_USB_OHCI_HCD=y
+CONFIG_USB_EHCI_HCD=y
+CONFIG_USB_KEYBOARD=y
+CONFIG_USB_STORAGE=y
+CONFIG_SYS_USB_EVENT_POLL_VIA_INT_QUEUE=y
-- 
2.31.0

