# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Radxa Zero"
deviceinfo_manufacturer="Radxa"
deviceinfo_codename="radxa-zero"
deviceinfo_dtb="amlogic/meson-g12a-radxa-zero"
deviceinfo_year="2021"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_gpu_accelerated="true"
deviceinfo_chassis="embedded"
deviceinfo_keyboard="true"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1920"
deviceinfo_screen_height="1080"

# Bootloader related
deviceinfo_flash_method="none"
deviceinfo_kernel_cmdline="rw console=ttyAML0,115200 console=tty0 no_console_suspend"
deviceinfo_sd_embed_firmware_step_size="512"
deviceinfo_sd_embed_firmware="u-boot/radxa-zero/u-boot.bin.sd-stripped.bin:1"
deviceinfo_boot_part_start="4096"
deviceinfo_generate_extlinux_config="true"
