# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Samsung Galaxy SL"
deviceinfo_manufacturer="Samsung"
deviceinfo_codename="samsung-i9003"
deviceinfo_year="2011"
deviceinfo_external_storage="true"
deviceinfo_flash_method="heimdall-bootimg"
deviceinfo_arch="armv7"

# Device related
deviceinfo_chassis="handset"
deviceinfo_keyboard="false"
deviceinfo_screen_width="480"
deviceinfo_screen_height="800"
deviceinfo_dev_touchscreen="/dev/input/event2"

# Offsets for the boot.img
deviceinfo_generate_bootimg="true"
deviceinfo_kernel_cmdline="console=ttySAC2,115200 buildvariant=userdebug"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x1000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x00000100"
deviceinfo_flash_pagesize="4096"

# Heimdall related
deviceinfo_flash_heimdall_partition_kernel="NORMALBOOT"
deviceinfo_flash_heimdall_partition_rootfs="SYSTEM"
