# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Libre Computer AML-S805X-AC-V1.0"
deviceinfo_manufacturer="Libre Computer"
deviceinfo_codename="librecomputer-lafrite"
deviceinfo_year="2019"
deviceinfo_dtb="amlogic/meson-gxl-s805x-libretech-ac"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_chassis="embedded"
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
deviceinfo_gpu_accelerated="true"
deviceinfo_screen_width="800"
deviceinfo_screen_height="600"

# Bootloader related
deviceinfo_flash_method="none"
deviceinfo_boot_filesystem="fat32"
deviceinfo_generate_extlinux_config="true"
deviceinfo_sd_embed_firmware_step_size="512"
deviceinfo_sd_embed_firmware="u-boot/librecomputer-lafrite/u-boot.bin.sd-stripped.bin:1"
deviceinfo_boot_part_start="4096"
deviceinfo_kernel_cmdline="console=null"
