# Maintainer: Dang Huynh <danct12@disroot.org>
pkgname=wl1251-cal
pkgver=1.2
pkgrel=1
pkgdesc="Retrieve wl1251 calibration data from a CAL partition and feed it to the driver"
url="https://github.com/maemo-leste/wl1251-cal"
arch="armv7"
license="LGPL-2.1-only"
makedepends="linux-headers"
subpackages="$pkgname-openrc"
triggers="$pkgname.trigger=/lib/firmware/ti-connectivity"
source="$pkgname-$pkgver.tar.gz::https://github.com/maemo-leste/wl1251-cal/archive/refs/tags/$pkgver.tar.gz
	wl1251-cal.initd
	calibrate-wl1251"
options="!check" # No tests

build() {
	make
}

package() {
	make install DESTDIR="$pkgdir"
	install -Dm755 "$srcdir/calibrate-wl1251" "$pkgdir/usr/bin/calibrate-wl1251"
	install -Dm755 "$srcdir"/wl1251-cal.initd "$pkgdir"/etc/init.d/wl1251-cal
}

openrc() {
	default_openrc
	install="$subpkgname.post-install"
}

sha512sums="
1a402553fc98fa8f2d81d34a548f96be91d13bdcb77ec8e9d8373732b27a6e908895f6044aef8e88dbcd9fa6fa04f0a3d62bed877be91ba6207f68440c3ce758  wl1251-cal-1.2.tar.gz
1793a4d09ce3c4f2af7b7b4e171ed04e4d5e70d3e40f365ef169879d2431bd1f7abe8702a422efb4d86449a2800b53c531af7353d4e4c2563985c97030cbd99b  wl1251-cal.initd
0d843727da4d2f3e2fe76ff80c68e67b85fa1e4797ba822d323f3b005df853ec5206c812a9e0caed96aff2bf5f353df79b20f1970c6382d90e02dc664411d0b4  calibrate-wl1251
"
