From 46ee4de1b5c5099e937ffa0dc044390e4455c3b3 Mon Sep 17 00:00:00 2001
From: Nikita Travkin <nikita@trvn.ru>
Date: Thu, 7 Sep 2023 15:02:35 +0500
Subject: [PATCH 1/8] remoteproc: qcom: pas: Add sc7180 adsp

sc7180 has a dedicated ADSP similar to the one found in sm8250.
Add it's compatible to the driver reusing the existing config so
the devices that use the adsp can probe it.

Signed-off-by: Nikita Travkin <nikita@trvn.ru>
Reviewed-by: Stephen Boyd <swboyd@chromium.org>
Link: https://lore.kernel.org/r/20230907-sc7180-adsp-rproc-v3-2-6515c3fbe0a3@trvn.ru
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
---
 drivers/remoteproc/qcom_q6v5_pas.c | 1 +
 1 file changed, 1 insertion(+)

diff --git a/drivers/remoteproc/qcom_q6v5_pas.c b/drivers/remoteproc/qcom_q6v5_pas.c
index b5447dd2dd35..55fafc68200e 100644
--- a/drivers/remoteproc/qcom_q6v5_pas.c
+++ b/drivers/remoteproc/qcom_q6v5_pas.c
@@ -1161,6 +1161,7 @@ static const struct of_device_id adsp_of_match[] = {
 	{ .compatible = "qcom,qcs404-adsp-pas", .data = &adsp_resource_init },
 	{ .compatible = "qcom,qcs404-cdsp-pas", .data = &cdsp_resource_init },
 	{ .compatible = "qcom,qcs404-wcss-pas", .data = &wcss_resource_init },
+	{ .compatible = "qcom,sc7180-adsp-pas", .data = &sm8250_adsp_resource},
 	{ .compatible = "qcom,sc7180-mpss-pas", .data = &mpss_resource_init},
 	{ .compatible = "qcom,sc7280-mpss-pas", .data = &mpss_resource_init},
 	{ .compatible = "qcom,sc8180x-adsp-pas", .data = &sm8150_adsp_resource},
-- 
2.43.2

