# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Google Pixel 3a XL"
deviceinfo_manufacturer="Google"
deviceinfo_codename="google-bonito"
deviceinfo_dtb_sdc="qcom/sdm670-google-bonito-sdc"
deviceinfo_append_dtb="true"
deviceinfo_year="2019"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_chassis="handset"
deviceinfo_keyboard="false"
deviceinfo_external_storage="false"
deviceinfo_screen_width="1080"
deviceinfo_screen_height="2160"

# Bootloader related
deviceinfo_flash_method="fastboot"
deviceinfo_generate_bootimg="true"
deviceinfo_bootimg_qcdt="false"
deviceinfo_bootimg_mtk_mkimage="false"
deviceinfo_bootimg_dtb_second="false"
deviceinfo_flash_pagesize="4096"
deviceinfo_flash_offset_base="0x00000000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x01000000"
deviceinfo_flash_offset_second="0x00000000"
deviceinfo_flash_offset_tags="0x00000100"
deviceinfo_flash_sparse="true"

# Reported to be necessary to boot sometimes on Android 9 bootloaders
deviceinfo_flash_fastboot_partition_vbmeta="vbmeta"

# Google Inc. Nexus/Pixel Device (tether)
deviceinfo_usb_idVendor="0x18d1"
deviceinfo_usb_idProduct="0x4ee3"

# Additional features
deviceinfo_flash_kernel_on_update="true"
deviceinfo_gpu_accelerated="true"
deviceinfo_super_partitions="/dev/mmcblk0p68 /dev/mmcblk0p69"
