# Based on arch/arm64/boot/dts/qcom/spi-panel-gc9305-hlt-24-qvga-cmd.dtsi from
# the downstream kernel, which is:
# Copyright (c) 2017, 2020, The Linux Foundation. All rights reserved.
#
# This program is free software; you can redistribute it and/or modify
# it under the terms of the GNU General Public License version 2 and
# only version 2 as published by the Free Software Foundation.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.

command 0xfe
command 0xfe
command 0xef
command 0x35 0x00
command 0x36 0x48
command 0x3a 0x05
command 0x20
command 0x38
command 0x13
command 0xa4 0x44 0x44
command 0xa5 0x42 0x42
command 0xa6 0x2a 0x2a
command 0xa7 0x2b 0x2b
command 0xa8 0x18 0x18
command 0xa9 0x2a 0x2a
command 0xaa 0x88 0x88
command 0xac 0x00
command 0xaf 0x55
command 0xe1 0x10 0x26
command 0xe3 0x01 0x10
command 0xe8 0x11 0x77
command 0xe0 0x0f
command 0xe4 0x00
command 0xe5 0x00
command 0xe6 0x00
command 0xe7 0x00 0x00
command 0xea 0x51 0x95 0x00 0x00 0x00 0x00 0x00
command 0xeb 0x30
command 0xec 0x33 0x22 0x88
command 0xed 0x18 0x08
command 0xee 0x00
command 0xa0 0x00
command 0xa1 0x00
command 0xa2 0x00
command 0xa3 0x00
command 0xab 0x00 0x00
command 0xad 0x33
command 0xae 0x2b
command 0xde 0x00
command 0xff 0x61
command 0xdf 0x08
command 0xb6 0x00 0x80 0x27
command 0xf0 0x02 0x01 0x00 0x00 0x03 0x07
command 0xf1 0x01 0x01 0x00 0x02 0x06 0x0e
command 0xf2 0x08 0x06 0x32 0x03 0x04 0x46
command 0xf3 0x10 0x0c 0x3e 0x06 0x03 0x4f
command 0xf4 0x0b 0x16 0x15 0x1d 0x1e 0x0f
command 0xf5 0x08 0x15 0x15 0x1b 0x1c 0x0f
command 0xfd 0x00
command 0x2a 0x00 0x00 0x00 0xef
command 0x2b 0x00 0x00 0x01 0x3f
command 0x44 0x00 0x40

command 0x11 # exit sleep mode
delay 120
command 0x29 # display on
