# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Motorola Moto G 4G (2013)"
deviceinfo_manufacturer="Motorola"
deviceinfo_codename="motorola-peregrine"
deviceinfo_year="2013"
deviceinfo_dtb_mainline="qcom-msm8926-motorola-peregrine"
deviceinfo_append_dtb_mainline="true"
deviceinfo_arch="armv7"

# Device related
deviceinfo_chassis="handset"
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
deviceinfo_screen_width="720"
deviceinfo_screen_height="1080"
deviceinfo_dev_touchscreen="/dev/input/event3"

# Bootloader related
deviceinfo_flash_method="fastboot"
deviceinfo_kernel_cmdline_downstream="androidboot.bootdevice=msm_sdcc.1 androidboot.hardware=qcom vmalloc=400M androidboot.selinux=permissive"
deviceinfo_generate_bootimg="true"
deviceinfo_generate_extlinux_config="true"
deviceinfo_bootimg_qcdt_downstream="true"
deviceinfo_flash_offset_base="0x10000000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x01000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x00000100"
deviceinfo_flash_pagesize="2048"
