# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="PINE64 A64-LTS"
deviceinfo_manufacturer="PINE64"
deviceinfo_codename="pine64-a64lts"
deviceinfo_date=""
deviceinfo_dtb="allwinner/sun50i-a64-pine64-lts"
deviceinfo_modules_initfs=""
deviceinfo_arch="aarch64"
deviceinfo_disable_dhcpd="true"

# Device related
deviceinfo_keyboard="true"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1024"
deviceinfo_screen_height="600"
deviceinfo_dev_touchscreen=""
deviceinfo_dev_touchscreen_calibration=""
deviceinfo_dev_keyboard=""

# Bootloader related
deviceinfo_flash_method="none"
deviceinfo_generate_legacy_uboot_initfs="true"
deviceinfo_sd_embed_firmware="u-boot/pine64-lts/u-boot-sunxi-with-spl.bin:8"
