# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="QEMU arm"
deviceinfo_manufacturer="QEMU"
deviceinfo_codename="qemu-vexpress"
deviceinfo_date=""
deviceinfo_keyboard="true"
deviceinfo_nonfree="????"
deviceinfo_dtb="vexpress-v2p-ca9"
deviceinfo_append_dtb="true"
deviceinfo_modules_initfs="amba-clcd virtio_net virtio_mmio ambakmi libps2 pcips2 qxl drm_bochs"
deviceinfo_external_storage="true"
deviceinfo_flash_method="none"
deviceinfo_generate_legacy_uboot_initfs="false"
deviceinfo_arch="armv7"
deviceinfo_kernel_cmdline="console=ttyAMA0,38400n8 console=tty1 PMOS_NO_OUTPUT_REDIRECT PMOS_FORCE_PARTITION_RESIZE"

# Splash
deviceinfo_screen_width="640"
deviceinfo_screen_height="480"
