From f1fa9be3da588eb045bf73a3de29b67fc7004062 Mon Sep 17 00:00:00 2001
From: Sergey Larin <cerg2010cerg2010@mail.ru>
Date: Thu, 7 Feb 2019 13:30:45 +0300
Subject: [PATCH] ARM: dts: tegra20-glide: fix duplicate i2c bus address

Camera and power i2c buses use separate addresses for operation.

Signed-off-by: Sergey Larin <cerg2010cerg2010@mail.ru>
---
 arch/arm/boot/dts/tegra20-glide.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm/boot/dts/tegra20-glide.dts b/arch/arm/boot/dts/tegra20-glide.dts
index 46e4d30b077a..93a4f50f0710 100644
--- a/arch/arm/boot/dts/tegra20-glide.dts
+++ b/arch/arm/boot/dts/tegra20-glide.dts
@@ -552,7 +552,7 @@
 		};
 	};
 
-	i2c@7000d000 {
+	i2c@7000c500 {
 		status = "okay";
 		clock-frequency = <400000>;
 
-- 
2.22.0

