# Reference: <https://postmarketos.org/devicepkg>
# Contributor: Alexey Min <alexey.min@gmail.com>
pkgname="device-samsung-klte"
pkgdesc="Samsung Galaxy S5"
pkgver=0.3
pkgrel=2
url="https://postmarketos.org"
license="MIT"
arch="armv7"
options="!check !archcheck"
depends="postmarketos-base mkbootimg msm-fb-refresher"
makedepends="devicepkg-dev"
subpackages="
	$pkgname-kernel-downstream:kernel_downstream
	$pkgname-kernel-mainline:kernel_mainline
	$pkgname-nonfree-firmware:nonfree_firmware
	$pkgname-nonfree-userland:nonfree_userland
	$pkgname-hybris:hybris
	$pkgname-hybris-x11:hybris_x11
"
source="
	deviceinfo
	fstab.android
	set-brightness
	battery-status
	70-klte-android.rules
	NetworkManager-klte.conf
"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname
}

kernel_downstream() {
	pkgdesc="Display, touchscreen, Wi-Fi works (see device table for details)"
	depends="linux-samsung-klte firmware-samsung-klte"
	install="$pkgname-kernel-downstream.post-install"

	devicepkg_subpackage_kernel $startdir $pkgname $subpkgname

	# Disable v4l udev rules (video4linux), because without the camera
	#         firmware blobs this makes udev helper hang (#1033)
	mkdir -p "${subpkgdir}"/etc/udev/rules.d
	ln -s /dev/null "${subpkgdir}"/etc/udev/rules.d/60-persistent-v4l.rules

	# NetworkManager configuration - ignore unsupported devices for now and set default dhcp client
	install -Dm644 "${startdir}/NetworkManager-klte.conf" \
		"${subpkgdir}/etc/NetworkManager/conf.d/10-klte.conf"

	# Extras, helper scripts that make life of developer/user easier
	install -Dm755 "${startdir}/set-brightness"          "${subpkgdir}/usr/bin/set-brightness"
	install -Dm755 "${startdir}/battery-status"          "${subpkgdir}/usr/bin/battery-status"
}

kernel_mainline() {
	pkgdesc="For kernel development only (most features aren't working)"
	depends="linux-postmarketos-qcom-msm8974"
	devicepkg_subpackage_kernel $startdir $pkgname $subpkgname
}

nonfree_firmware() {
	pkgdesc="Wifi firmware"
	depends="firmware-samsung-klte"
	mkdir "$subpkgdir"
}

nonfree_userland() {
	pkgdesc="Pulls libhybris (Android) hardware adaptation"
	depends="$pkgname-hybris"
	mkdir "$subpkgdir"
}

hybris () {
	pkgdesc="libhybris (Android) hardware adaptation"
	depends="hybris-base"
	install="$pkgname-hybris.post-install"

	mkdir "$subpkgdir"

	# Android mounts (needed for loading firmware and configs from android container)
	# Appended to fstab in post-install script
	install -Dm644 "${startdir}/fstab.android"           "${subpkgdir}/etc/fstab.android"

	# Android udev rules, depend on android users and groups presence
	install -Dm644 "${startdir}/70-klte-android.rules" \
		"${subpkgdir}/etc/udev/rules.d/70-klte-android.rules"
}

hybris_x11() {
	pkgdesc="x11 modules for libhybris adaptation"
	depends="hybris-base-x11-caf"
	install_if="$pkgname-hybris xorg-server"

	mkdir "$subpkgdir"
}

sha512sums="334b57770c4b0e78e385b3c8a30eb4fad9eea88fed3ddbe7d82341b600feae5418feda6c3afc4ef57bb0a870996c4f249f449cced2a5d952da80158cd7e2c632  deviceinfo
35f3b120152ebe709e11cebc9ced03f21f52768d88bd68ed23ed864fe1dd3b63665c8f74575882e217dd8226ae5d260e5ad2045dc4ab2470c89185f19b81c4a7  fstab.android
f773a9792407c1ad96b11c6673093c9eeff7d538459b7772c5956760a8cbb4de8912b24c77e8812afe056db26fa3e29af09e2a3851828baa0b9a9986bf80790b  set-brightness
66db173b9f1075a133efeea8bda94ef08089b7c15acbc1e3aefb9f8510daa7690a0ce2739d20647e096ba69940ac5c4c6699f3b032ec67609ca56f116bb25256  battery-status
a68734d3fe30695d5a9302c92327e8ca564a73d06f0de87371800d1bdf4c541c3721af380b8d44cfa0b4cc1dc8a71586aec3f00bb877ee9dc18f41ba34caaeff  70-klte-android.rules
3753dcd8c25cfbbdd8f087a3168537df1334f0d33f36bc8923ec3d225ceb88121aa8d1670d6c6a2baab3d7067c86a43571695ce22e3b47076f97fcb53d1d7e6f  NetworkManager-klte.conf"
