From db4e9ffdb985752ae3c3436ff86f8f376ae8fd22 Mon Sep 17 00:00:00 2001
From: Tobias Schramm <t.schramm@manjaro.org>
Date: Thu, 28 May 2020 14:25:32 +0200
Subject: [PATCH] phy: rockchip: typec: Set extcon capabilities

Do not mainline, hack.

Signed-off-by: Tobias Schramm <t.schramm@manjaro.org>
---
 drivers/phy/rockchip/phy-rockchip-typec.c | 17 +++++++++++++++++
 1 file changed, 17 insertions(+)

diff --git a/drivers/phy/rockchip/phy-rockchip-typec.c b/drivers/phy/rockchip/phy-rockchip-typec.c
index 70a31251b202..5385bb4f0bd4 100644
--- a/drivers/phy/rockchip/phy-rockchip-typec.c
+++ b/drivers/phy/rockchip/phy-rockchip-typec.c
@@ -40,6 +40,7 @@
 #include <linux/clk-provider.h>
 #include <linux/delay.h>
 #include <linux/extcon.h>
+#include <linux/extcon-provider.h>
 #include <linux/io.h>
 #include <linux/iopoll.h>
 #include <linux/kernel.h>
@@ -1160,6 +1161,22 @@ static int rockchip_typec_phy_probe(struct platform_device *pdev)
 				dev_err(dev, "Invalid or missing extcon\n");
 			return PTR_ERR(tcphy->extcon);
 		}
+	} else {
+		extcon_set_property_capability(tcphy->extcon, EXTCON_USB,
+					       EXTCON_PROP_USB_SS);
+		extcon_set_property_capability(tcphy->extcon, EXTCON_USB_HOST,
+					       EXTCON_PROP_USB_SS);
+		extcon_set_property_capability(tcphy->extcon, EXTCON_DISP_DP,
+					       EXTCON_PROP_USB_SS);
+		extcon_set_property_capability(tcphy->extcon, EXTCON_USB,
+					       EXTCON_PROP_USB_TYPEC_POLARITY);
+		extcon_set_property_capability(tcphy->extcon, EXTCON_USB_HOST,
+					       EXTCON_PROP_USB_TYPEC_POLARITY);
+		extcon_set_property_capability(tcphy->extcon, EXTCON_DISP_DP,
+					       EXTCON_PROP_USB_TYPEC_POLARITY);
+		extcon_sync(tcphy->extcon, EXTCON_USB);
+		extcon_sync(tcphy->extcon, EXTCON_USB_HOST);
+		extcon_sync(tcphy->extcon, EXTCON_DISP_DP);
 	}
 
 	pm_runtime_enable(dev);
-- 
GitLab 
