# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="PINE64 PineTab"
deviceinfo_manufacturer="PINE64"
deviceinfo_codename="pine64-pinetab"
deviceinfo_year="2019"
deviceinfo_dtb_allwinner="allwinner/sun50i-a64-pinetab"
deviceinfo_dtb_allwinner_dev="allwinner/sun50i-a64-pinetab-dev"
deviceinfo_modules_initfs=""
deviceinfo_arch="aarch64"

# Device related
deviceinfo_gpu_accelerated="true"
deviceinfo_chassis="tablet"
deviceinfo_keyboard="true"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1280"
deviceinfo_screen_height="800"
deviceinfo_framebuffer_landscape="true"
deviceinfo_getty="ttyS0;115200"
deviceinfo_mesa_driver="sun4i-drm"
deviceinfo_dev_internal_storage="/dev/mmcblk2"
deviceinfo_dev_internal_storage_repartition="true"

# Bootloader related
deviceinfo_flash_method="none"
deviceinfo_generate_legacy_uboot_initfs="true"
deviceinfo_sd_embed_firmware="u-boot/pine64-pinephone/u-boot-sunxi-with-spl-528.bin:8"

# USB related
deviceinfo_usb_idVendor="0x1f3a"   # Allwinner Technology Co., Ltd.
deviceinfo_usb_idProduct="0x1007"  # unknown (same as stock Android on PineTab)
