# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Teclast X80 Pro"
deviceinfo_manufacturer="Teclast"
deviceinfo_codename="teclast-x80pro"
deviceinfo_year="2017"
deviceinfo_dtb=""
deviceinfo_modules_initfs="i915 usbhid usb-storage hid_generic sdhci_acpi mmc_block xhci_pci sd_mod"
deviceinfo_arch="x86_64"

# Device related
deviceinfo_gpu_accelerated="true"
deviceinfo_chassis="tablet"
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1200"
deviceinfo_screen_height="1920"
deviceinfo_dev_touchscreen="/dev/input/event5"

# Bootloader related
# See wiki for this device. Installation procedure is non-standard.
deviceinfo_flash_method="none"
